SERVICE MANUAL UPDATE-SEC. 8A I/P & INTERIOR LAMPS, WIRING. GMC Truck S15 Pickup - 4WD 1993

For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 8A I/P & INTERIOR LAMPS, WIRING

#### SUBJECT: SECTION 8A INSTRUMENT PANEL AND INTERIOR LAMPS, WIRING COLOUR/CONNECTOR CHANGES

#### VEHICLES AFFECTED: 1993 BRAVADA

The following represents new and/or revised information for Section 8A-81 (Instrument Panel) and 8A-l 14 (Interior Lamps) of the 1993 Bravada Service Manual.

#### Section 8A-81 has the following changes.

Page 8A-81-3. Wire colour in fuel gage description was changed from PNK to PPL.

Page 8A-81-6. Wire designation on fuel gage circuit changed from .8 TAN 31 to .8 PPL 30.

Page 8A-81-6. Location of connector C402 updated.

Section 8A-114 has the following changes.

Page 8A-114-2. Connector C205A was added.

Page 8A-l14-3. Corrected terminal I.D. at the I/P Courtesy Lamp, RH, and a page reference below that has been corrected.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.