ACCUMULATOR SPRING THM 700-R4 TRANSMISSION. GMC Truck S15 Pickup - 4WD 1983

For 1990-2009 cars

# ACCUMULATOR SPRING THM 700-R4 TRANSMISSION

#### MODELS: 1982-1983 LIGHT DUTY TRUCKS WITH THM 700-R4 TRANSMISSION

The following charts show the correct 1-2 and 3-4 accumulator spring usage for all 1982 and 1983 THM 700-R4 transmissions. See Figure No. 1 for proper spring location.

1982 THM 700-R4

#### Models 1-2 Accumulator Spring 3-4 Accumulator Spring

Color Part Number Color Part Number

YK, YL, Y3, Y4 Violet 8634163 Green 8634162

T5, T6, TW, TC, TE, TH, TJ, TK, TN, TP, Green 8634162 Green 8634162 YA, MB, MC, MD, ME, MH, M2, M4, M5, M6, M7, Y6

1983 THM 700-R4

#### Models 1-2 Accumulator Spring 3-4 Accumulator Spring

Color Part Number Color Part Number

YN, YK, YP, T8, TZ, TS, MH, VJ, TL Violet 8634163 Red 8634703

VA, PQ, YH, ML, MP, MS, T7. YF, YG, Y9, TC, MB, MC, MJ, VN, Red 8634703 Red 8634703 TE, TH, TK, MD, ME, MK, MW, VH, TP

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.