PAINT IDENTIFICATION ASSEMBLY PLANT. GMC Truck S15 Pickup - 4WD 1988

For 1990-2009 cars

# PAINT IDENTIFICATION ASSEMBLY PLANT

#### MODELS: ALL 1988 LIGHT AND MEDIUM DUTY TRUCK MODELS

Attached is a current listing of the various assembly plants and their paint suppliers. It should be noted, however, that paint suppliers are subject to change at any given time.

Assembly Plants Plant Paint Paint Type Trucks Code Supplier ---------- --------------- ----- -------- Basecoat/Clearcoat Baltimore, Maryland B PPG Enamel

Basecoat/Clearcoat Fort Wayne, Indiana Z Dupont Enamel

Basecoat/Clearcoat Pontiac East, Michigan E Dupont Enamel

Basecoat/Clearcoat Oshawa, Ontario 1 CIL Waterborne

Acrylic Enamel Scarborough, Ontario 4 CIL High Solids Enamel Flint, Michigan F Inmont High Solids Enamel Janesville, Wisconsin J Dupont High Solids Enamel Lordstown, Ohio 7 Inmont High Solids Enamel Moraine, Ohio 2 Inmont High Solids Enamel Pontiac-Central, Michigan V Inmont Dupont AKZO High Solids Enamel Pontiac-West, Michigan 0 Inmont High Solids Enamel Shreveport, Louisiana 8 Inmont

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.