1989 PAINT CODES ALL TRUCKS. GMC Truck S15 Pickup - 2WD 1989

For 1990-2009 cars

# 1989 PAINT CODES ALL TRUCKS

#### MODELS: ALL 1989 TRUCK MODELS

The following is a list of paint code numbers from various suppliers for the 1989 model year. These colors can be obtained locally.

DuPont refinish paints are avilable in:

L - Lucite(R) - Acrylic Lacquer A - Centari(R) - Acrylic Enamel D - Dulux(R) - Enamel 355S - Flexible Additive 1234 Vinyl Lacquer - Chip resistant

#### IMPORTANT: Vinyl resin must be added to the base color when painting interior components.

DuPont vinyl resin #304 - instrument panel. DuPont vinyl resin #305 - all rem aining interior parts except seats. DuPont vinyl resin #306 - seats and vinyl roofs.

When ordering DuPont paint, use "L", "A", "D", 355S or 1234 with the appropriate DuPont code.

Ditzler refinish paints are available in: DDL - Duracryl - Acrylic Lacquer DBU - Deltron - B/C

DAR - Delstar - Acrylic Enamel DAU - Deltron - Acrylic Urethane UCV - Vinyl Colors DX - 369 - Flexative - Flexible Finishes DX-54 - Roadguard - Road Abrasion Protection

When ordering PPG paint, use "DDL", "DBU", "DAR", "DAU", "UCV", "DX-369" or "DX-54" with appropriate Ditzler code.

Sherwin-Williams, Acme/Rogers, and Martin- Senour are available in acrylic lacquer or acrylic enamel.

S-Wuse: prefix 34, J4 or L10 for acrylic lacquer, prefix 35, J5 or F10 for acrylic enamel.

Acme use: prefix 84 for acrylic lacquer, prefix 85 for acrylic enamel.

Rogersuse:prefix 94 for acrylic lacquer, prefix 95 for acrylic enamel.

Martin-Senour:jobber will interchange number shown when acrylic lacquer is needed.

***1989 Truck Exterior and Interior Paint Colors***

#### 1989 TRUCK EXTERIOR COLORS

Paint Sherwin- Color Color Name Fisher DuPont Martin Williams PPG Rinshed Code ---------- W-Code ------ -Senour Acme-Rogers DDL/DAR Mason ---- ------ ------- ----------- ------- ----- 10 White B/C 9225 B8796 36783 36783 4015 18121 12 White 5111 817 30-3563 LlOA-1369 2185 1347 1492 15 Silver Metallic B/C 8914 C8501 32-5452 34856 3794 15251 17 Slate Metallic 7468 B8235 30-5142 32377 3453 12866 18 Black Metallic B/C 9150 B8789 36443 36443 4005 18113 19 Black 5118 99S 3069 LlOB-1738 9000 Standard 3O00/4590 /9300 Package 20 Black B/C 8555 99S 30-5296 33756 9700 13572 21 Light Blue Metallic 7470 B8237 30-5143 32378 3455 12868 23 Medium Blue 7154 B8041 30-4907 30527 3250 11500 24 Bright Blue Metallic 9222 B8894 38144 38144 4110 18120 27 Light Blue Metallic 9264 B8944 39337 39337 4146 19031 28 Dark Blue Metallic 8264 B8461 30-5332 34073 3685 14240 29 Dark Blue 7349 B8139 30-5079 31514 3362 12238 33 Light Mesa Brown 9207 B8945 39338 39338 4152 19028 34 Light Mesa Brown 9208 B8895 38145 38145 4107 18116 Metallic 35 Medium Mesa Brown 9201 B8941 40379 40379 4179 19025 36 Dark Hunter Green 9210 B8896 38146 38146 4108 18117 Metallic 37 Light Mesa Brown 9219 B8897 38147 38147 4111 18118 40 Dark Mesa Brown 9202 B8942 40380 40380 4180 19026 Metallic 42 Bright Blue 9203 B8943 40381 40381 16813 19027 44 Forest Green Metallic 7964 D8801 30-5539 35441 4114 15366 46 Woodland Green 7156 B8046 30-4912 30530 3255 11505 50 White B/C 8624 B8550 32-5455 34851 3800 15255 52 Gold Metallic B/C 9008 B8738 36345 36345 3917 17113 58 Light Sandstone 8865 B8792 36450 36450 4020 18111 Metallic B/C 61 Tan 8265 B8462 30-5329 34070 3686 14241 62 Light Sandstone 8817 B8740 36451 36451 4007 17115 67 Saddle Metallic 8799 B8630 30-5489 35342 3914 - 68 Dark Saddle Metallic 9212 B8741 36452 36452 4001 17116 70 Red B/C 8832 B8793 36453 36453 - - 71 Red Orange 7753 B8250 30-5146 32384 - 12884 72 Bright Red 7475 B8241 30-5120 32097 3464 12885 74 Red 9260 B8946 39339 39339 4154 19030 75 Red Metallic B/C 8919 C8506 32-5459 34855 3804 15259 77 Dark Gamet Red 9154 B8742 36454 36454 4002 17117 Metallic B/C 78 Dark Maple Metallic 8800 B8632 32-5524 35366 3915 16117 79 Dark Camine 8066 45827 30-4846 30086 3164 9890 80 Slate Gray 7382 B8207 30-5099 31993 3442 12687 83 Gumnetal Metallic B/C 8915 C8502 32-5467 35082 3805 15260 86 Wheatland Yellow 9014 B8743 32-8545 35586 3911 15616 87 Wheatland Yellow 5247 43536 30-4761 LIOY-3952 2785 2876 25511 88 Tangier Orange 5108 31 30-4760 LlOE-3953 60156 1597 25512 89 Tangier Orange 9013 B8744 30-5550 35587 3912 15617 90 Gray Metallic 8789 B8629 30-5490 35367 3916 16118 93 Polar White 5704 4074 32-4445 LlOA-3553 2680 4430 11691 95 Gamet Red Metallic B/C 8815 B8794 36456 36456 4022 18110 96 Silver Metallic B/C 8867 B8795 36457 36457 4023 18112 98 Black Saphire Metallic 8863 B8745 36458 36458 4003 17118 B/C B/C Basecoat/Clearcoat

#### 1989 TRUCK INTERIOR COLORS

Sherwin- GM Gloss Fisher Martin- Williams Trim Color Name Semi Flat W-Code Senour Acme- Code ---------- ---- ---- ------ ------ Rogers ---- ------ 12DN Graphite X 7701 16963 33767 X 16905 2989 16CN Dark Gray X 7773 16940 33237 X 17117 34995 18DN Dark Charcoal X 7350 16851 31901 X 17113 34991 19N Black X J4-8677 848 16615 92387 X 33024 23CN Medium Blue X 7151 16741 30820 X 17111 34989 23DN Dark Blue X 7163 16742 30821 X 17112 34990 24CN Dark Blue X 9059 36478 36478 X 39838 39838 24DN Very Dark Blue X 8576 17075 34606 17067 34598 6OBN Medium Cognac X 9205 38393 38393 38394 38394 6OCN Dark Cognac X 9099 38392 38392 X 38395 38395 6ODN Very Dark X 9252 38391 38391 Cognac X 38396 38396 62DN Dark Saddle X 8257 16969 33773 X 16951 33716 69BN Medium Beige X 8248 16966 33770 X 16950 33715 69CN Medium Dark X 8280 17074 34605 Beige X 17066 34597 77DN Dark Maple X 7298 16803 31423 X 17032 33780 77EN Very Dark Maple X 8284 16970 33774 X 16953 33718 8781 17134 35433 X 17147 35468 78DN Very Dark X 8827 36500 36500 Gamet Red X 36473 36473 82CN Medium Dark X 16965 33769 Gray X 8247 16949 33714

82DN Dark Gray X 8595 17080 34611 X 17071 34602

GM Gloss PPG Trim Color Name Semi FlAT PPG Vinyl Rinshed Code ---------- ---- ---- DIA Interior Mason DuPont ---- Code UCV Code ----- ------ ---- --- ---- 12DN Graphite X 33622 2-1020 13199 C8345 X 14028 16CN Dark Gray X 33871 2-1012 16067 C8586 X 16068 18DN Dark Charcoal X 33872 2-871 12730 C8575 X 14030 19N Black X 4401 9640 120 C8535 X 12812 23CN Medium Blue X 15951 2-770 11535 C8576 X 11593 23DN Dark Blue X 15953 2-765 11594 C8002 X 11595 24CN Dark Blue X 16323 2-1276 17124 C8792 X 19021 24DN Very Dark Blue X 15886 2-1098 15080 C8539 16045 6OBN Medium Cognac X 26281 2-1292 18055 C8808 19022 6OCN Dark Cognac X 26284 2-1315 18056 C8810 X 18057 6ODN Very Dark X 26285 2-1316 18058 C8819 Cognac X 18059 62DN Dark Saddle X 25354 2-1086 - C8579 X 69BN Medium Beige X 14006 C8446 X - - 17120 69CN Medium Dark X - - 15065 C8554 Beige X 77DN Dark Maple X 72700 2-803 12271 C8538 X 12391 77EN Very Dark Maple X 72596 2-1089 14026 C8581 X 72799 2-1173 16055 C8616 X 17085 78DN Very Dark X 51247 2-1222 17092 D8747 Gamet Red X 17089 82CN Medium Dark X 33665 14009 C8447 Gray X 2-1048 14088 15268 82DN Dark Gray X 33824 2-1125 15095 C8550 X

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.