1993 PAINT CODES, SUPPLIERS, ASSY. PLANT ID-(SERVICE INFO). GMC Truck S15 Pickup - 2WD 1993

For 1990-2009 cars

# 1993 PAINT CODES, SUPPLIERS, ASSY. PLANT ID-(SERVICE INFO)

#### SUBJECT: 1993 PAINT CODES, PAINT SUPPLIERS AND ASSEMBLY PLANT IDENTIFICATION

#### MODELS: 1993 ALL MODEL TRUCKS

THIS BULLETIN CANCELS AND REPLACES GMC TRUCK SERVICE BULLETIN 93-10-7, DATED SEPTEMBER 1992 TO ADD TRUCK EXTERIOR AND INTERIOR PAINT COLORS. ALL COPIES OF 93-10-7 SHOULD BE DESTROYED.

Attached is a current listing of the various assembly plants and their paint suppliers. It should be noted, however, that paint suppliers are subject to change at any given time.

Paint Type Assembly Plant Plant Paint (Trucks) Code Supplier ------------------ -------------- ------ -------- Basecoat/Clearcoat Baltimore, MD B PPG Enamel (M/L)

High Solids Janesville, WI J Dupont Enamel (MD)

Basecoat/Clearcoat Flint, MI (G) F BASF Enamel

High Solids Moraine, OH 2 Dupont Enamel (S/T)

Basecoat/Clearcoat Oshawa Truck 1 PPG Waterborne Plant (C/K)

High Solids Pontiac-West, 0 BASF Enamel MI (S/T)

Basecoat/Clearcoat Pontiac-East, MI E Dupont Enamel (C/K)

Medium Solids Scarborough, 4 PPG Enamel Ontario (G)

High Solids Shreveport, LA 8 BASF Enamel (S/T)

Basecoat/Clearcoat Ft. Wayne, IN Z Dupont Enamel (C/K)

Basecoat/Clearcoat Janesville, WI J PPG Enamel (C/K - Surburban Yukon, Sierra Crew Cab)

The following is a list of paint code numbers from various suppliers for the 1993 model year. These colors can be obtained locally.

1. BASF refinished paints are available in: A-Alphacryl D-Diamont 88 SO-Diamont Solo 21-Glasurit-21 54-Glasurit-54 S-Limco Select L-Limco Supreme Gold M-Miracryl Super Max

#### Flexible Finishes

When spraying flexible plastic parts, use the following recommendation:

Elastifier additive 521-111 for Vinyl application when using Glasurit 54 and 21 lines.

891 Flex Agent for Vinyl Application when using Alphacryl, Miracryl, Diamont 88, and Supreme Gold.

DF-25 for Vinyl application when using Diamont Solo.

#### NOTE: When using a basecoat/clearcoat system only use the flex agent in the clearcoat application.

#### Stone Chip Protector

Glassohyd 1109-1240/6 Stone Chip Protector is a waterborne material which uses a durable, flexible plastic dispersion as its bonding media. This product is versatile in application and may be easily applied by spray, brush, or roller. When Glassohyd is completely cured, the material is resis- tant to water, gasoline, and oil. Glassohyd has excellent stone impact and corrosion resistance. Glassohyd Stone Chip Protector can be topcoated directly with 21-line or 54/94-line colors.

II. DuPont refinished paints are available in: - L-Lucite-Acrylic Lacquer - A-Centari-Acrylic Enamel - J-Cronar-Polyoxithane Enamel - K-Chromabase(TM) - 350S-Flexlar-Flexible Additive - 310S-Black-1-2-3 Vinyl Lacquer - 33OS-White-1-2-3 Vinyl Lacquer - V-Lucite Vinyl

#### Important

Vinyl resin must be added to the base color when painting interior components.

DuPont vinyl resin 304S (instrument panel).

DuPont vinyl resin 305S (all remaining interior parts except seats).

DuPont vinyl resin 306S (seats and vinyl roofs).

When ordering DuPont paint, use "L", "A", "J", "K" or "V" with the appropriate DuPont Code.

III. PPG (Ditzler) refinish paints are available in: - DDL-Duracryl-Acrylic Lacquer or Acrylic Basecoat/Clearcoat - DBU-Deltron-Basecoat/Clearcoat - DAR-Delstar-Acrylic Enamel - DAU-Deltron-Acrylic Urethane - UCV-Vinyl Colors - DX-369-Flexative-Flexible Finishes - DX-54-Roadguard-Road Abrasion Protection

When ordering PPG (Ditzler) paint, use "DDL", "DBU", "DAR", "DAU", "UCV", "DX-54", or "DX-369" with appropriate Ditzler code.

IV. Sherwin-Williams, Acme/Rogers, and Martin-Senour are available in acrylic lacquer, acrylic enamel, or acrylic urethane.

S-W use: o prefix 34, J4 or L10/L11 for acrylic lacquer, o prefix 35, J5 or F10/F11 for acrylic enamel, o prefix UB for acrylic urethane in a basecoat/clearcoat system, o prefix US for acrylic urethane in a single stage system

ACME use: o prefix 84 for acrylic lacquer, o prefix 85 for acrylic enamel, o prefix PB for acrylic urethane in a basecoat/clearcoat system o prefix PS for acrylic urethane in a single stage system.

Rogers Use: o prefix 94 for acrylic lacquer, o prefix 95 for acrylic enamel, o prefix AU for acrylic urethane in a basecoat/clearcoat system o prefix AS for acrylic urethane in a single stage system.

Martin-Senour:o Jobber will interchange number shown when acrylic lacquer is needed, o use prefix 98 for acrylic urethane as an inter-mix basecoat/clearcoat, o use prefix 88 for acrylic urethane as a factory packaged basecoat/clearcoat, o use prefix 97 for acrylic urethane as an inter-mix single stage system, o use prefix 87 for acrylic urethane as a factory packaged single stage system.

1993 TRUCK EXTERIOR COLORS

GM WA COLOR NAME NO. NO. ---------------------- BASF Glasurit Martin- Sherwin- PPG Rinshed 54-21 Acme- DuPont Senour Williams DDI-DAR Mason Line Rogers ------ ------- -------- ------- ------- ------- ------- 10 9225 GHOST WHITE AE660 36783 36783 4015 18121 GM-9225 36782

12 5111 LINEN WHITE 21667 82-1208 F8W-2030 2815 1347 GM-5438 1492

14 8915 GUNMETAL AC547 90-5973 35082 3805 15260 GM-8915 35082

15 8914 ASTRAL SILVER AC546 82-5915 34856 3796 15251 GM-7054 34856

16 9659 WARM GRAY MET DF243 44149 44149 4314 21017 GM-9659 44149

17 7468 LT SLATE MET AK903 82-5579 32377 12866 GM-7023 32377

18 9017 DOVE GRAY DF856 46962 46962 35567 23020 GM-9017 46962

19 5118 LAMP BLACK 78400 8800 F8B-1738 9000/9300 PKG 21-1240 80

20 9790 LT QUASAR BLUE MET DF840 46963 46963 4714 23004 GM-9790 46963

22 9656 BAHAMA BLUE MET DF242 44150 44150 4307 21018 GM-9656 44150

23 7154 OCEAN BLUE BR007 82-5258 30527 3250 11500 GM-5481 30527

24 9222 MEDIUM BLUE MET AD933 38144 38144 4110 18120 GM-9222 38144

26 9662 PASTEL BLUE DF702 44151 44151 4308 21019 GM-9662 44151

27 9264 LT FRENCH BLUE MET AE682 39337 39337 4146 19031 GM-9264 39337

28 8863 BLACK SAPPHIRE MET AD924 36458 36458 4003 17118 GM-8863 36458

29 7349 DK BLUE BR106 82-5448 31514 3362 12283 GM-5039 31514

33 9207 LT MESA BROWN AD926 39338 39338 4152 19028 GM-9207 39338

34 9793 LT TEAL MET DF862 45878 45878 4455 22072 GM-9793 45878

36 9828 MED DK TEAL MET DF864 45879 45879 4347 22073 GM-9828 45879

38 9794 BRIGHT TEAL MET DF836 46964 46964 4716 22265 GM-9794 46964

39 9792 INDIGO MET DF857 46965 46965 4717 23006 GM-9792 46965

41 8555 BLACK AB921 82-5760 33756 9700 13572 54-1240 33756

44 7964 FOREST GREEN MET AH792 90-6024 35441 4114 15366 GM-7964 35441

46 7156 DK GREEN BR008 82-5263 30530 3255 11505 GM-5482 30530

47 9095 DK BLUE MET DF525 42479 42479 4251 20052 GM-9095 42479

48 9096 DK RED DF526 42480 42480 4239 20053 GM-9096 42480

50 8624 OLYMPIC WHITE AC301 82-5918 34851 3800 15255 GM-8624 34851

52 9087 KHAKI DF853 46966 46966 4718 23021 GM-9087 46966

54 9831 SPRUCE MET DF861 45913 45913 4500 22267 GM-9831 45913

57 5400 BEIGE MET DF778 45881 45881 4346 22271 GM-5400 45881

61 8265 TAN AB415 82-5799 34070 3686 14241 GM-1074 34070

71 7753 RED ORANGE AB153 82-5586 32384 3463 12884 GM-3046 32384

72 7475 STANDARD RED AK412 82-5539 32097 3464 12885 GM-3047 32097

74 9260 VICTORY RED AE737 39339 39339 4154 19030 GM-9030 39339

75 8919 RED MET AC557

76 9154 DK GARNET RED MET AE068 36454 36454 4002 17117 GM-9154 36454

78 8800 MAROON MET AC605 99-6069 35366 16117 GM-3091 35366

80 9791 MED QUASAR BLUE MET DF839 46967 46967 4719 23022 GM-9791 46967

83 9916 RADISSON RED MET 46968 46968 4720 23023 GM-9916 46968

84 9927 DK HUNT CLUB RED MET DF842 46969 46969 4721 23007 GM-9927 46969

90 8798 GRAY MET AC603 82-6001 35367 16118 GM-8793 35367

91 6270 DK ARGENT DF863 22223 GM-22223

96 8867 ULTRA SILVER MET AD911 36457 36457 4023 18112 GM-8867 36457

97 9658 DARK GRAY MET DF244 44153 44153 4313 21047 GM-9658 44153

1993 TRUCK INTERIOR COLORS

| | | | |Sherwin-| | PPG | | GM | |Gloss | | |Williams|PPG |Vinyl |(BASF)| Trim| | |Fisher|Martin|Acme- |DIA |Interior|Rinshed Code|Color Name |Semi Flt|W-Code|Senour|Rogers |Code |UCV Code|Mason |DuPont ----------------------------------------------------------------------------- 12DN|GRAPHITE | X |7701 | | |33622|2-1020 |16042 | | | X |7701 | | |33870|2-1020 |13199 | | | | | | | | | | 13AN|LT SMOKE | X |9653 |44438 |44437 |35203|2-1441 |21026 |C9109 |GRAY | X |9653 |44438 |44437 |35204|2-1441 |21029 |C9110 | | | | | | | | | 13BN|MED SMOKE | X |9654 |44439 |45940 |35205|2-1442 |21027 |C9110 |GRAY | | | | | | | | | | | | | | | | | 13CN|DK SMOKE | X |9655 |45941 |44440 |35206|2-1443 |21028 |C9111 |GRAY | | | | | | | | | | | | | | | | | 18DN|DK CHARCOAL| X |7350 |16851 |131901 |33872|2-871 |14030 |C8575 | | X |7350 |17113 |34991 |33492|2-871 |12730 |C8575 | | | | | | | | | | | | | |J4-8677/| | | | 19DN|BLACK | X |848 |16615 |92387 |9640 |2-120 |12812 |C8535 | | X |848 |16918 |33024 |9433 |2-120 |4401 |C8535 | | | | | | | | | 24CN|DARK BLUE | X |9059 |36478 |39838 |16323|2-1276 |19021 |C8792 | | X |9059 |36478 |39838 |16323|2-1276 |17124 |C8792 | | | | | | | | | 24DN|VERY DK | X |8576 |17075 |34606 |15886|2-1098 |16045 |C8539 |BLUE | X |8576 |17067 |34598 |16092|2-1098 |115080|C8539 | | | | | | | | | 24EN|MIDNT BLUE | X |9541 |42600 |42599 |16998|2-1396 |20066 |C9006 | | X |9541 |42600 |42599 |16999|2-1396 |20065 |C9006 | | | | | | | | | 47CN|DARK RED | X |9104 |42602 |42601 |73381|2-1394 |20062 |C9007 | | X |9104 |42602 |42601 |73380|2-1394 |20061 |C9007 | | | | | | | | | 47DN|VERY DK RED| X |9253 |42604 |42603 |73383|2-1395 |22274 |C9008 | | X |9753 |42604 |42603 |73382|2-1395 |20063 |C9008 | | | | | | | | | 60BN|MED COGNAC | X |9205 |38394 |138393 |26281|2-1292 |19022 |C8808 | | X |9205 |38394 |38393 |26281|2-1292 |18055 |C8808 | | | | | | | | | 60CN|DARK COGNAC| X |9099 |38395 |38392 |26284|2-1315 |18057 |C8810 | | X |9099 |38395 |38392 |26284|2-1315 |18056 |C8810 | | | | | | | | | 64AN|LIGHT BEIGE| X |9776 |45943 |45942 |27307|2-1477 |22251 |C9230 | | X |9776 |45943 |45942 |27307|2-1477 |22276 |C9230 | | | | | | | | | 64BN|MED BEIGE | X |9777 |45945 |45944 |27312|2-1478 |22277 |C9231 | | X |9777 |45945 |45944 |27308|2-1478 |22278 |C9231 | | | | | | | | | 64DN|DARK BEIGE | X |9778 |45947 |45946 |27313|2-1479 |22279 |C9232 | | X |9778 |45947 |45946 |27309|2-1479 |22280 |C9232 | | | | | | | | |

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.