Automatic Level Control Connector End Views. Opel Sintra 1999

For 1990-2009 cars

Table 1: | Auto Level Control (ALC) Air Compressor (With Inflator)
Table 2: | Auto Level Control (ALC) Air Compressor (Without Inflator)
Table 3: | Auto Level Control (ALC) Inflator Relay
Table 4: | Auto Level Control (ALC) Sensor (With Inflator)
Table 5: | Auto Level Control (ALC) Sensor (Without Inflator)
Table 6: | Inflator Air Switch

#### Auto Level Control (ALC) Air Compressor (With Inflator)

Connector Part Information

• | 12059472

• | 7-Way F Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 43 | Fused battery feed
B | WHT | 320 | Auto level control air compressor vent solenoid output
C | ORN | 1240 | Fused battery feed
D | YEL | 321 | Auto level control compressor relay output-coil
E | ORN | 1240 | Fused battery feed
F | -- | -- | Not Used
G | BLK | 1725 | Ground

#### Auto Level Control (ALC) Air Compressor (Without Inflator)

Connector Part Information

• | 12059472

• | 7-Way F Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 39 | Fused battery feed
B | WHT | 320 | Auto level control air compressor vent solenoid output
C | ORN | 1240 | Fused battery feed
D | YEL | 321 | Auto level control compressor relay output-coil
E | ORN | 1240 | Fused battery feed
F | -- | -- | Not Used
G | BLK | 1725 | Ground

#### Auto Level Control (ALC) Inflator Relay

Connector Part Information

• | 02965977

• | 8-Way F 56 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 1267 | Auto level control reset signal
B | LT BLU | 1248 | Auto level control height sensor
C | DK BLU | 1249 | Auto level control solenoid valve feed
D | ORN | 1240 | Fused battery feed
E | YEL | 321 | Auto level control compressor relay output-coil
F | WHT | 1245 | Auto level control inflator switch output
G | -- | -- | Not Used
H | BLK | 1725 | Ground

#### Auto Level Control (ALC) Sensor (With Inflator)

Connector Part Information

• | 12052848

• | 6-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1725 | Ground
B | YEL | 321 | Auto level control compressor relay output-coil
C | LT BLU | 1248 | Auto level control height sensor
D | YEL | 43 | Fused ignition 1 feed
E | WHT | 320 | Auto level control air compressor vent solenoid output
F | -- | -- | Not Used

#### Auto Level Control (ALC) Sensor (Without Inflator)

Connector Part Information

• | 12052848

• | 6-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1725 | Ground
B | YEL | 321 | Auto level control compressor relay output-coil
C | ORN | 1240 | Fused battery feed
D | PNK | 39 | Fused ignition 1 feed
E | WHT | 320 | Auto level control air compressor vent solenoid output
F | -- | -- | Not Used

#### Inflator Air Switch

Connector Part Information

• | 12015683

• | 3-Way F Pin Grip Connector (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 1245 | Auto level control inflator switch output
B | BLK | 1725 | Ground
C | PPL | 1267 | Auto level control reset signal