Power Mirrors Inoperative. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire outside mirrors system check performed? | -- | Go to Step 2 | Go to Outside Mirrors System Check
2 | Backprobe with a test light from the outside rearview mirror remote control switch connector terminal E and ground. Does the test light illuminate? | -- | Go to Step 3 | Go to Step 4
3 | Using a test light, backprobe between the outside rearview mirror remote control switch connector terminal E and terminal D. Does the test light illuminate? | -- | Go to Step 5 | Go to Step 6
4 | Repair the open or poor connection in CKT 1140. Is the repair complete? | -- | Go to Step 7 | --
5 | Replace the outside rearview mirror remote control switch. Refer to Door Trim Plate Replacement . Is the repair complete? | -- | Go to Step 7 | --
6 | Repair the open in circuit 750 from S504 to the outside rearview mirror remote control switch connector terminal D Is the repair complete? | -- | Go to Step 7 | --

7

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all the repairs been made?

--

Go to Outside Mirrors System Check

--