Front Side Door Inside Handle Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the front door inside handle from the lock rod.
4. Unsnap the front door inside handle from the lock module in order to remove the front door inside handle from the door.

### Installation Procedure

1. Snap the front door inside handle to the lock module in order to install the front door inside handle to the door.
2. Install the front door inside handle to the lock rod.
3. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .