Automatic Transmission Components. Opel Sintra 1999

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Automatic Transaxle | Lower left side of the engine compartment | -- | --
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Brake Transmission Shift Lock Control Actuator (BTSI) | Inside steering column near ignition switch | -- | --
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | --
Ignition Switch | Part of the steering column | -- | --
Left Taillamp | Rear of the vehicle, left side | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Rear Side Door Actuator Control Module | Part of the rear side door actuator motor, right quarter panel, above the wheelhouse | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Rear Side Door Actuator Motor | Right quarter panel, above the wheelhouse | -- | --
Right Taillamp | Rear of the vehicle, right side | -- | Lighting Systems Connector End Views in Lighting Systems
Starter Solenoid | Lower front of the engine, part of the starter motor assembly | Automatic Transmission Electronic Component Views in Automatic Transmission | --
Stop Lamp Switch | Mounted to the brake pedal support | Antilock Brake System Component Views in ABS/Traction Control | Cruise Control Connector End Views in Cruise Control
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Automatic Transmission Electronic Component Views in Automatic Transmission | Engine Controls Connector End Views in Engine Controls
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Vehicle Speed Sensor (VSS) | Lower right tear of the engine compartment, mounted to the right side of the transaxle | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
C101 (10 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, next to C103 and C181 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C103 (2 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, next to C101 and C181 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C111 (7 cavities) | Engine wiring harness to the automatic transaxle wiring harness, lower left side of the engine compartment, front of the automatic transaxle | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G113 | Engine compartment, left of the starter, along with the battery ground | Harness Routing Views in Wiring Systems | --
G402 | Secured to the lower right D-pillar | -- | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views in Wiring Systems | --
P400 | Behind the right taillamp | Harness Routing Views in Wiring Systems | --
P401 | Behind the left taillamp | Harness Routing Views in Wiring Systems | --
S106 | Engine harness, front left side of the engine compartment approximately 10 cm (4 in) from the PCM breakout | -- | --
S122 | Engine harness, top left side of the radiator approximately 25 cm (10 in) from the engine coolant fan 1 (right) motor breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --
S406 | Body harness, left rear of the body approximately 17 cm (7 in) from the P401 breakout | -- | --