Rear Fog Lamps Always On. Opel Sintra 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the rear fogIamp system check performed? | -- | Go to Step 2 | Go to Fog Lights System Check

2

1. Turn the headlamp and I/P lamp dimmer switch to the OFF position.
2. Disconnect the rear fog lamp relay.

Are the rear fog lamps still on?

--

Go to Step 3

Go to Step 4

3 | Repair a short to voltage on CKT 122. Has the repair been made and the system rechecked? | -- | System OK | --
4 | Use a DMM in order to probe the rear fog lamp relay connector terminal C1 and ground. Is the resistance within the specified range? | 0-2ohms | Go to Step 5 | Go to Step 6
5 | Repair a short to ground on CKT 1870. Has the repair been made and the system rechecked? | -- | System OK | --
6 | Replace the rear fog lamp relay. Has the repair been made and the system rechecked? | -- | System OK | --