Output Shaft Replacement. Opel Sintra 1997

For 1990-2009 cars

### Removal Procedure

#### Tool Required

J 34757 Snap Ring Tool

1. Remove the case extension housing. Refer to Case Extension Replacement .
2. Remove the output shaft retaining clip at the differential.
3. Remove the output shaft through the left wheel opening.
4. Inspect the output shaft for damage.

### Installation Procedure

1. Install the output shaft through the left wheel opening.
2. Install the output shaft retaining clip at the differential.
3. Install the case extension housing. Refer to Case Extension Replacement .