Rear Seat Back Recliner Cover Replacement. Opel Sintra 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the recliner cover screws.
2. Unsnap the covers (4) from the recliner starting from the rear of the cover.

### Installation Procedure

1. Snap the cover (3) to the recliner starting from the front of the cover.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the recliner cover screws.

Tighten
Tighten the recliner cover screws to 2 N·m (18 lb in).