Tilt Wheel/Column Components. Opel Sintra 1999

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Brake Transmission Shift Lock Control Actuator | Inside the steering column, near the ignition switch | -- | --
BTSI/TCC Brake Switch | Mounted to the brake pedal support, connector 2 of the stop lamp switch | -- | --
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | --
Stop Lamp Switch | Mounted to the brake pedal support | Antilock Brake System Component Views in ABS/Traction Control | Cruise Control Connector End Views in Cruise Control
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Automatic Transmission Electronic Component Views in Automatic Transmission | Engine Controls Connector End Views in Engine Controls
C101 (10 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, next to C103 and C181 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G113 | Engine compartment, left of the starter, along with the battery ground | Harness Routing Views in Wiring Systems | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views in Wiring Systems | --
S106 | Engine harness, front left side of the engine compartment approximately 10 cm (4 in) from the PCM breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --