Engine Electrical Components. Opel Sintra 1999

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Battery | Engine compartment, behind the right headlamp | -- | --
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | --
Fusible Link A | Bolted to the starter solenoid | Automatic Transmission Electronic Component Views in Automatic Transmission | --
Fusible Link Z | Bolted to the starter solenoid | Automatic Transmission Electronic Component Views in Automatic Transmission | --
Generator (K68) | Top rear right side of the engine | Engine Controls Component Views in Engine Controls | Engine Electrical Connector End Views in Engine Electrical
Generator (KG9) | Top rear right side of the engine | Engine Controls Component Views in Engine Controls | Engine Electrical Connector End Views in Engine Electrical
Ignition Switch | Part of the steering column | -- | --
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Security Indicator Lamp | Center of the IP, mounted to the trim plate, near the windshield defrost vent | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Starter Motor | Lower front of the engine | Automatic Transmission Electronic Component Views in Automatic Transmission | --
Starter Solenoid | Lower front of the engine, part of the starter motor assembly | Automatic Transmission Electronic Component Views in Automatic Transmission | --
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Automatic Transmission Electronic Component Views in Automatic Transmission | Engine Controls Connector End Views in Engine Controls
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
C103 (2 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, next to C101 and C181 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G100 | Battery grounded to the right inner fender, near the battery | Harness Routing Views in Wiring Systems | --
G113 | Engine compartment, left of the starter, along with the battery ground | Harness Routing Views in Wiring Systems | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --