V6 DIESEL FUEL FILTER SERVICE PARTS- NB9 FILTER SYSTEM. Pontiac LeMans 1982

For 1990-2009 cars

# V6 DIESEL FUEL FILTER SERVICE PARTS- NB9 FILTER SYSTEM

PARTS TO SERVICE THE DIESEL FUEL FILTER ASSEMBLY USED ON THE V6 DIESEL ENGINE WERE NOT RELEASED INTO THE SERVICE PARTS SYSTEM. THE PARTS SHOWN BELOW ARE NOW AVAILABLE TO SERVICE THE DIESEL FUEL FILTER ASSEMBLY. OWNERS SHOULD BE REMINDED THAT THE FUEL FILTER CARTRIDGE IS TO BE REPLACED EVERY 30,000 MILES (48,000 KM) AS INDICATED IN THE MAINTENANCE SCHEDULE. A/C NO. WDDGM PART NO. DESCRIPTION T101 25011844 FUEL FILTER COMPLETE ASSEMBLY WITHOUT HEATER T101H 25011843 FUEL FILTER COMPLETE ASSEMBLY WITH HEATER TP1000 25011603 FUEL FILTER OF1007 25011836 HEATER PACKAGE FOR FILTER OF1008 25011837 WATER DETECTOR ELECTRONICS

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.