HOOD WOBBLES WHEN OPEN DUE TO LOOSE HINGE PIVOT BOLTS. Pontiac Sunbird 1988

For 1990-2009 cars

# HOOD WOBBLES WHEN OPEN DUE TO LOOSE HINGE PIVOT BOLTS

#### Models Affected: 1988-89 SUNBIRD

Some 1988-89 Sunbirds may have hood bolts that have insufficient loctite and could loosen. This will allow the hood to have a loose wobbly feel when opened. This condition has been corrected in production at the following VIN breakpoints:

LE 1G2JB11K8K7594520 4/14/89 Lordstown SE 1G2JD11KXK7598224 4/22/89 Lordstown GT 1G2JU11M4K7598219 4/14/89 Lordstown

To repair this condition, install new hinge pivot bolts, part number 22548097. Parts are currently available through GMSPO. Refer to the illustration for identification (the new bolt has a hex head).

#### Warranty Information:

Labor Operation Number: T4654 Labor Time : 0.4 hrs both

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.