LTG. REQUEST FOR REVIEW CHANGE 1988 JUNE,JULY, AND AUGUST. Pontiac Sunbird 1988

For 1990-2009 cars

# LTG. REQUEST FOR REVIEW CHANGE 1988 JUNE,JULY, AND AUGUST

"Please discard bulletin 88-WA-11, dated 9/88, due to being published with an incorrect bulletin number, the correct number is shown above."

This bulletin addresses changes to the published Pontiac Labor Time Guide, June through August changes attached. These changes are the result of dealer "Requests For Review" being handled by C-P-C Technical Service Activity.

These updates will be included in future 1988 Labor Time Guide revisions. In the case of past model year updates, it is recommended that this bulletin be retained with all appropriate model year Labor Time Guides, as a complete revision will not be provided.

REQUEST FOR REVIEW Vehicle Series OPERATION DESCRIPTION OPEWION A B F H J N T W NUMBER VIN CODE EFGH L SW XYZ BDU EVW NRSX JKP

FINESSE SAND AND BUFF A0110 .3 .3 .3 .3 .3 .3 .3 .3 NOTE: Total time not to exceed .5 hours. Applicable to 1989 models. ADD: A- For Each Additional Panel .1 .1 .1 .1 .1 .1 .1 .1

LATCH, VISTA VENT GLASS B2200 .3 - ALIGN OR REPLACE NOTE: Applicable model year 1989

RETAINER, VISTA VENT B2215 .4 - REPLACE NOTE: Applicable model year: 1989

HINGE, VISTA VENT GLASS - R&R OR REPLACE NOTE:Applicable model year: 1989 RIGHT B2220 .2 LEFT B2221 .2 BOTH B2227 .2

AIR DEFLECTOR, ROOF OPENING B2230 .4 - REPLACE NOTE: Applicable model year: 1989

GLASS, VISTA VENT - REPLACE B2240 .2 NOTE: Applicable model year: 1989

ESCUTCHEON, VISTA VENT B2245 .2 - REPLACE NOTE: Applicable model year: 1989

LACE, VISTA VENT OPENING B2250 .2 FINISHING - REPLACE NOTE: Applicable model year: 1989 ADD: A- To Color Coat .2 GB

FRAME, VISTA VENT - REPLACE B2278 2.8 NOTE: Applicable model year: 1989

PANEL, SUNROOF SLIDING GLASS B2760 .4 - REPLACE NOTE: Applicable model years: 1988-89

HOUSING ASSEMBLY, SUNROOF B2780 1.0 (MODULE) - REPLACE NOTE: Applicable model years: 1988-89

LOCATOR, DRIVE CABLE AND/OR B2800 .3 MICRO SWITCH - REPLACE NOTE: Applicable model years: 1988-89

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N T W NUMBER VIN CODE EFGH L SW XYZ BDU EVW NRSX JKP

BRACKET, SIDE ADJUSTMENT B2810 .6 - REPLACE NOTE: Applicable model years: 1988-89

CABLE, SUNROOF DRIVE B2820 1.3 - R&R OR REPLACE NOTE: Applicable model years: 1988-89

GUIDE, SUNROOF SLIDING B2840 .7 PANEL SIDE - R&R OR REPLACE NOTE: Applicable model years: 1988-89

CHANNEL DRAIN - REPLACE B2850 .5 NOTE: Applicable model years: 1988-89

SUNSHADE, SUNROOF B2900 .5 SLIDING GLASS PANEL - R & R or REPLACE NOTE: Applicable model years:1988-89

EMBLEM, FENDER OR DOOR - REPLACE NOTE: Applicable model year: 1988

RIGHT B7400 .2 LEFT B7401 .2

REGULATOR, FRONT DOOR WINDOW - R&R OR REPLACE NOTE: Applicable model years: All RIGHT POWER C0182 1.0 LEFT POWER C0183 1.0

LOCK CONSOLE COMPARTMENT C2700 .2 - R&R OR REPLACE NOTE: Applicable model years: 1987-88

HANDLE, SEAT ADJUSTER C6150 .2 - REPLACE NOTE: Applicable model years: 1987-88

HOSES, AIR DISTRIBUTION - R&R OR REPLACE NOTE: Applicable model years: 1987-88 TO RIGHT SIDE DEFROSTER D1544 .3 TO LEFT SIDE DEFROSTER D1545 .3

SEALL REFRIGERANT 'O' RING - REPLACE NOTE: Applicable model year: 1988 EVAPORATOR INLET LINE D3051 .5 EVAPORATOR OUTLET LINE D3052 .5

PUMP AND/OR GASKET, J3480 2.0 COOLANT - REPLACE NOTE: Applicable model years: 1987-88 w/ V-6

REQUEST FOR REVIEW

Vehicle Series OPERATION DESCRIPTION OPERATION A B F H J N T W NUMBER VIN CODE EFGH L SW XYZ BDU EVW NRSX JKP

SHIELD, FUEL INJECTOR J5643 .2 SIGHT - REPLACE NOTE: Applicable model year: 1988

ELECTRONICALLY CONTROLLED EMISSIONS AND FUEL SYSTEM - REPLACE SENSOR EXHAUST OXYGEN J6372 .6 NOTE: Applicable model year: 1988

COVER AND/OR GASKET, TRANSMISSION SHIFT - R&R OR REPLACE K2240 3.0 NOTE: Applicable model years: 1985-89 ADD: A- To Recondition Cover .4

TRANSMISSION ASSEMBLY K2700 2.6 - RECONDITION NOTE: Applicable model years: 1985-89 ADD: A- To Recondition Shifter Cover .8 B- To Replace Main Drive Gear Bearing .3 Retainer And/Or Gasket C- To Replace Main Drive Gear Bearing .5 D- To Recondition Main Shaft 1.8 E- To Replace Case Extension And Seal .6 F- To Replace Speedometer Drive Gear .4 G- To Replace Bell Housing .5 H- To Replace Case 1.6 I- To Recondition Trans Assy 3.2

#### NOTE: Total add time not to exceed 'Recondition Trans Assy' add time.

TRANSMISSION ASSEMBLY K2720 2.9 - REPLACE NOTE: Applicable model years: 1985-89

COVER AND/OR GASKET, K6540 1.9 VALVE BODY REPLACE NOTE: Applicable model year: 1987

HORN ASSEMBLY - REPLACE N0200 .4 NOTE: Applicable model year: 1988

SWITCH - REPLACE NOTE:Applicable model year:1988 STOP LAMP N2440 .5

REQUEST FOR REVIEW VEHICLES SERIES OPERATION DESCRIPTION OPERATION A B F H J N T W NUMBER VIN CODE EFGH L SW XYZ BDU EVW NRSX JKP

MOTOR - REPLACE NOTE: Applicable model years: All DOOR WINDOW RIGHT FRONT N3314 1.0 LEFT FRONT N3315 1.0

LUGGAGE RACK COMPONENTS - REPLACE

#### NOTE: Applicable model years: 1987-89

BRACKET AND/OR BAR R2320 .4

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F H J N P T W NUMBER VINCO EFGH L SW XYZ BDU EVW EFGM NRSX JKP

FINESSE SAND AND BUFF A0110 .3 .3 .3 .3 .3 .3 .3 .3 .3 NOTE: Total time not to exceed .5 hours. Applicable to 1988 models. ADD: A- For Each Additional Panel .1 .1 .1 .1 .1 .1 .1 .1 .1

MANIFOLD, EXHAUST J0108 1.1 - REPLACE NOTE: Applicable model years: 1984-86 w/ L-4

PUMP AND/OR GASKET, J3480 2.1 COOLANT - REPLACE NOTE: Applicable model years: 1985-88 w/ V-6

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.