FRT. STEERING KNUCKLE/HUB ASSY SUSPENSION MODIFICATION. Pontiac Sunbird 1984

For 1990-2009 cars

# FRT. STEERING KNUCKLE/HUB ASSY SUSPENSION MODIFICATION

Some late production 1984 Sunbirds were assembled with 1985 front steering knuckle and hub assemblies. These vehicles are identified below by assembly plant and VIN breakpoint.

#### VEHICLE IDENTIFICATION

Assembly Plant V.I.N. Breakpoint -------------- ----------------- Pontiac Lordstown E7345533 - Up

If servicing of these vehicles necessitates part replacement, usage of the applicable 1985 service parts noted below will be required.

#### 1985 Service Parts

Parts Parts Description Number ----------------- ------ Steering Knuckle (L. H.) 14066983

Steering Knuckle (R. H.) 14066984

Splash Shield (L. H.) 14066987

Splash Shield (R. H.) 14066988

Brake Rotor 14091771

Front Wheel Bearing Kit 7470004

Splash Shield Attaching Bolt 14035591

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.