1984 CARBURETOR ADJUSTMENT SPEC. REVISIONS. Pontiac Sunbird 1984

For 1990-2009 cars

# 1984 CARBURETOR ADJUSTMENT SPEC. REVISIONS

The Carburetor Model E2SE Adjustment Specifications have been revised and should replace the specifications given in the loose-leaf manual.

The revised specifications are included in the bound manuals.

1984 6000 and Phoenix Models Carburetor Model E2SE Adjustment Specifications

FAST IDLE VAC. CARB.# FLOAT LEAN IDLE AIR CHOKE CAM BREAK LEVEL MIXTURE MIXTURE VALVE COIL (CHOKE PRI. +/- 1/16" SCREW SCREW SPRING LEVER ROD) +/- 2.5 DEG in. mm (TURNS) (TURNS) (TURNS) +/- 3.5 DEG --- -- ----- ----- ----- ----- -------- --------

17084356 9/32 7.0 2 1/2 4 3/4 0.085 22 DEG 25 DEG 17083457 9/32 7.0 2 1/2 4 3/4 0.085 22 DEG 25 DEG 17084358 9/32 7.0 2 1/2 4 3/4 0.085 22 DEG 25 DEG 17084359 9/32 7.0 2 1/2 4 3/4 0.085 22 DEG 25 DEG 17084368 1/8 3.3 2 1/2 4 3/4 0.085 22 DEG 25 DEG 17084370 1/8 3.3 2 1/2 4 3/4 0.085 22 DEG 25 DEG 17084534 5/32 3.6 2 1/2 4 1/2 0.085 28 DEG 25 DEG 17084535 5/32 3.6 2 1/2 4 1/2 0.085 28 DEG 25 DEG 17084537 5/32 3.6 2 1/2 4 1/2 0.085 28 DEG 25 DEG 17084358 5/32 3.6 2 1/2 4 1/2 0.085 28 DEG 25 DEG 17084540 5/32 3.6 2 1/2 4 1/2 0.085 28 DEG 25 DEG 17084542 1/8 3.0 2 1/2 4 1/2 0.085 28 DEG 25 DEG 17084632 9/32 7.0 2 1/2 4 1/2 0.085 28 DEG 25 DEG 17084633 9/32 7.0 2 1/2 4 1/2 0.085 28 DEG 25 DEG 17084635 9/32 7.0 2 1/2 4 1/2 0.085 28 DEG 25 DEG 17084636 9/32 7.0 2 1/2 4 1/2 0.085 28 DEG 25 DEG

CARB.# ------- VALVE BREAK UNLOADER ROD SEC. +/- 6 DEG --- +/-3.5 DEG ---------- -----------

17084356 1 DEG 30 DEG 30 DEG 17083457 1 DEG 30 DEG 30 DEG 17084358 1 DEG 30 DEG 30 DEG 17084359 1 DEG 30 DEG 30 DEG 17084368 1 DEG 30 DEG 30 DEG 17084370 1 DEG 30 DEG 30 DEG 17084534 1 DEG 35 DEG 45 DEG 17084535 1 DEG 35 DEG 45 DEG 17084537 1 DEG 35 DEG 45 DEG 17084358 1 DEG 35 DEG 45 DEG 17084540 1 DEG 35 DEG 45 DEG 17084542 1 DEG 35 DEG 45 DEG 17084632 1 DEG 35 DEG 45 DEG 17084633 1 DEG 35 DEG 45 DEG 17084635 1 DEG 35 DEG 45 DEG 17084636 1 DEG 35 DEG 45 DEG

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.