RATTLE NOISE IN GLOVE BOX AREA TRIM ECM BRACKET AS OUTLINED. Pontiac Sunbird 1987

For 1990-2009 cars

# RATTLE NOISE IN GLOVE BOX AREA TRIM ECM BRACKET AS OUTLINED

1987 SUNBIRD MODELS

#### CONDITION:

--------- A rattle in glove box area of instrument panel.

#### CAUSE:

----- The ECM bracket contacts the glove box at the left edge.

#### CORRECTION:

----------- Refer to the Illustration and trim 15 mm of material off the top edge of the left side of the glove box as shown. This will provide the necessary clearance for the ECM bracket.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.