PULSE WIPER PHANTOM WIPE OXIDATION-WIPER SW.CONTACTS. Pontiac Sunbird 1984

For 1990-2009 cars

# PULSE WIPER PHANTOM WIPE OXIDATION-WIPER SW.CONTACTS

1984 2000 SUNBIRD WINDSHIELD PULSE WIPER

On some 1984 2000 Sunbirds, the windshield pulse wipers may cycle one or several times without the switch being turned on. This condition may be caused by oxidation or corrosion on the column wiper switch contacts. The condition can be repaired by replacing the switch with the following new switch numbers:

7848195 Non-Tilt Column 7848196 Tilt Column

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.