REVISED CYLINDER HEAD GASKET IMPROVED SEALING. Pontiac Sunbird 1987

For 1990-2009 cars

# REVISED CYLINDER HEAD GASKET IMPROVED SEALING

#### Models Affected: 1987 GRAND PRIX AND 1987-89 SAFARI AND FIREBIRD WITH 5.OL AND 5.7L ENGINES (VIN CODES F, H, 8 AND 6)

A cylinder head gasket with improved sealing characteristics is now available for service use on 5.OL and 5.7L (VIN Codes F, H, 8, and 6) engine applications. The applicable part numbers are listed below:

Cylinder Head Gasket Application Part Number ----------- --------------------

5.OL Engine 10105115

5.7L Engine 10105117

These parts are currently available from GMSPO.

Use applicable Labor Time and operation Number.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.