BINDING AUTOMATIC THM LINKAGE CORROSION200 & 200C. Pontiac T1000 1982

For 1990-2009 cars

# BINDING AUTOMATIC THM LINKAGE CORROSION200 & 200C

CORROSION MAY CAUSE BINDING OF SHIFT LINKAGE ON 1978-83 CHEVETTE AUTOMATIC TRANSMISSIONS. ADD LUBRICANT (SEE ILLUSTRATION) TO THE REAR SHIFTER ROD PIN AREA PER THE GENERAL MOTORS MAINTENANCE SCHEDULE. THIS PERIODIC LUBRICATION WILL PREVENT BINDING OF SHIFT LINKAGE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.