SERVICE MANUAL UPDATE SEC. 3C FRONT SUSPENSION HUB SEAL TOOL. Pontiac Tempest (Canada) 1991

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 3C FRONT SUSPENSION HUB SEAL TOOL

#### Subject: SERVICE MANUAL UPDATE - SECTION 3C FRONT SUSPENSION (INNER HUB SEAL INSTALLER ART WORK LABELED WITH CORRECT TOOL NUMBER)

#### Models Affected: 1991 SUNBIRD AND GRAND AM MODELS

The 1991 Sunbird and Grand Am Service Manual improperly labels the Inner Hub Seal Installer. The correct tool number is J 34658.

The following art for this tool #J34658 replaces the current art shown. Reference to the tool number must also be corrected on the following pages in the text.

PAGES TEXT ILLUSTRATION CARLINE ---------- ------------- -------- 3C-7, 3C-8 3C-14 Sunbird 3C-8, 3C-10 3C-16 Grand Am

Please correct your copies of the Service Manuals.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.