For 1990-2009 cars

### Removal Procedure

1. Remove the CD player trim plate. Refer to Front Floor Console Replacement in Instrument Panel, Gauges and Console.
2. Use a small, flat-bladed tool in order to release the CD player retainers.
3. Pull the CD player from the front floor console.
4. Disconnect the electrical connector.
5. Remove the CD player from the front floor console.

### Installation Procedure

1. Install the CD player to the front floor console.
2. Connect the electrical connector.
3. Push the CD player into the front floor console.

Ensure that the retainers lock into place.

4. Install the CD player trim plate. Refer to Front Floor Console Replacement in Instrument Panel, Gauges and Console.