For 1990-2009 cars

#### Ashtray Lamp Connector

Connector Part Information |

• | 12124722

• | W2 Axial Type Lamp Socket Wedge Base (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior lamp dim signal
B | BLK | 150 | Ground

#### Auxiliary Heater-A/C Control C1

Connector Part Information |

• | 12064978

• | 6-Way F Micro-Pack 100 Series (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | 641 | Fused ignition 3 feed
2 | GRY | 8 | Interior lamp dim signal
3 | GRY | 778 | Auxiliary blower motor switch output
4 | GRY | 773 | Transaxle range switch input C
5 | BLK | 955 | Rear temperature input
6 | BLK | 850 | Ground

#### Backup Lamp Relay

Connector Part Information |

• | 12110541

• | 6-Way F Metri-Pack 280 Series Flexlock (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | PNK | 539 | Fused ignition 1 feed
A2 | LT GRN/BLK | 24 | Backup lamp signal
B1-B2 | -- | -- | Not Used
C1 | LT GRN/BLK | 924 | Backup lamp feed
C2 | BLK | 1450 | Ground

#### Cargo Lamp

Connector Part Information |

• | 12047662

• | 2-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | GRY/BLK | 690 | Courtesy lights control output (GND)

#### Center High Mounted Stop Lamp (CHMSL)

Connector Part Information |

• | 12047662

• | 2-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 17 | Stop lamp switch output
B | BLK | 450 | Ground

#### Daytime Running Lamps (DRL) Ambient Light Sensor

Connector Part Information |

• | 12047662

• | 2-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 1137 | Daytime running lamp ambient light sensor signal
B | YEL/BLK | 1138 | Daytime running lamp ambient light sensor return

#### Daytime Running Lamps (DRL) Control Module C1

Connector Part Information |

• | 12064998

• | 8-Way F Metri-Pack 280 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1340 | Fused battery feed
B | LT BLU | 14 | Turn signal lamp feed-left front
C | DK BLU | 15 | Turn signal lamp feed-right front
D | YEL | 2340 | Fused battery feed
E | LT BLU/WHT | 1414 | Turn signal lamp feed-left front
F | YEL | 10 | Headlamp switch output
G | DK BLU/WHT | 1415 | Turn signal lamp feed-right front
H | BRN | 9 | Park lamp feed

#### Daytime Running Lamps (DRL) Control Module C2

Connector Part Information |

• | 12064766

• | 8-Way F Metri-Pack 150 Series (Blue)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1450 | Ground
B | -- | -- | Not Used
C | PNK | 1839 | Fused ignition 1 feed
D | TAN/WHT | 33 | Brake warning indicator lamp output
E | LT BLU | 1134 | Park brake switch signal
F | BRN | 241 | Fused ignition 3 feed
G | YEL/BLK | 1138 | Daytime running lamp ambient light sensor return
H | LT GRN/BLK | 1137 | Daytime running lamp ambient light sensor signal

#### Dome Lamp

Connector Part Information |

• | 12047662

• | 2-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | GRY/BLK | 690 | Courtesy lights control output (GND)

#### Hazard Lamp/Turn Signal Flasher

Connector Part Information |

• | 12110541

• | 6-Way F Metri-Pack 280 Series Flexlock (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | LT BLU | 1508 | Hazard lamp/turn signal flasher red
A2 | -- | -- | Not Used
B1 | -- | -- | Not Used
B2 | BLK | 1450 | Ground
C1 | PPL | 16 | Turn signal flasher output
C2 | -- | -- | Not Used

#### Headlamp and I/P Lamp Dimmer Switch

Connector Part Information |

• | 12059993

• | 17-Way Metri-Pack Mixed Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1450 | Ground
B | WHT | 156 | Courtesy lamp output
C-F | -- | -- | Not Used
G | BRN/WHT | 230 | Instrument panel lamps dimmer module output
H | GRY | 8 | Interior lamp dim signal
I | GRY/BLK | 308 | Park lamp switch output-parklamps ON
J-K | -- | -- | Not Used
L | YEL | 10 | Headlamp switch output
M | -- | -- | Not Used
N | ORN | 2340 | Fused battery feed
O | ORN | 1340 | Fused battery feed
P | LT BLU | 1872 | Park lamp switch signal-park lamps OFF
R | BRN | 0 | Park lamp feed

#### Heater-A/C Control (C60) C2

Connector Part Information |

• | 12064799

• | 12-Way F Micro-Pack 100 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 119 | Heater-A/C ON/OFF signal
B | DK GRN/WHT | 762 | A/C request signal
C | BRN | 241 | Fused ignition 3 feed
D | WHT | 193 | Rear defogger relay output-coil
E | ORN | 640 | Fused battery feed
F | PPL | 361 | Mode valve solenoid output-defrost
G | LT BLU | 733 | Temperature valve position signal
H | LT BLU | 684 | Air inlet valve signal
J | GRY | 8 | Interior lamp dim signal
K | BLK | 150 | Ground
L | WHT | 454 | Mode switch output
M | -- | -- | Not Used

#### Interior Lamp and Multi-function Switch C1

Connector Part Information |

• | 12162502

• | 8-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | 650 | Ground
2 | GRY | 8 | Interior lamp dim signal
3-4 | -- | -- | Not Used
5 | DK BLU | 1393 | Courtesy lamps feed-protected battery
6-7 | -- | -- | Not Used
8 | PPL | 328 | Interior lamp override switch output

#### Interior Lamp and Multi-function Switch C3

Connector Part Information |

• | 12041301

• | 8-Way F Metri-Pack 280 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior lamp dim signal
B | BLK | 650 | Ground
C | LT BLU | 1894 | Power sliding door switch signal
D | BLK/WHT | 1896 | Power sliding door system switch signal
E-H | -- | -- | Not Used

#### Interior Lamp and Multi-function Switch C4

Connector Part Information |

• | 12047976

• | 8-Way F Metri-Pack 380 Series (Blue)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | FRY | 8 | Interior lamp dim signal
B | BLK | 650 | Ground
C | BLK | 902 | Rear quarter window switch-open
D | BRN | 901 | Rear quarter window switch-close
E | BRN | 741 | Fused ignition 3 feed
F | ORN | 110 | Sunroof switch signal-close
G | DK BLU | 128 | Sunroof switch return
H | BRN | 100 | Sunroof switch signal-open

#### IP Compartment Lamp Switch

Connector Part Information |

• | 12124568

• | 2-Way M Lamp Socket Wedge Base STD (Natural)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 150 | Ground

#### Left Door Lock Switch

Connector Part Information |

• | 12089527

• | 6-Way F Metri-Pack 280 Series (LT Green)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 195 | Door lock switch input-battery
B | BLK | 750 | Ground
C | GRY | 8 | Interior lamp dim signal
D | WHT | 194 | Door unlock switch input-battery
E | BLK | 750 | Ground
F | -- | -- | Not Used

#### Left Front Door Lock C1 (Ajar Indicator Switch)

Connector Part Information |

• | 12162190

• | 4-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 159 | Key in ignition output
B | YEL | 804 | Door ajar indicator lamp output
C | -- | -- | Not Used
D | BLK | 750 | Ground

#### Left Front Fog Lamp

Connector Part Information |

• | 12124819

• | 2-Way F Metri-Pack 280 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 34 | Fog lamp feed
B | BLK | 1350 | Ground

#### Left Front Park/Turn Lamp

Connector Part Information |

• | 12160394

• | Right Angle Type W-3 Bulb Base Sealed (Natural)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 14 | Turn signal lamp feed-left front
B | BRN | 9 | Park lamp feed
G | BLK | 1350 | Ground

#### Left Front Side Marker

Connector Part Information |

• | 12110053

• | Axial Type W-2 Bulb Base Sealed (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 18 | Tail/turn/stop lamp feed-left rear
B | BRN | 9 | Park lamp feed

#### Left Headlamp

Connector Part Information |

• | 12048369

• | 3-Way F Metri-Pack 280 Series Sealed (Blue)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1350 | Ground
B | TAN | 12 | Low beam headlamp feed
C | LT GRN | 11 | High beam headlamp feed

#### Left IP Courtesy Lamp

Connector Part Information |

• | 12124652

• | W2 Axial Type Lamp socket Wedge Base (Clear)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | GRY/BLK | 690 | Courtesy lights control output (GND)

#### Left License Lamp

Connector Part Information |

• | 12110053

• | Type W-2 F Axial Bulb Base (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Park lamp feed
B | BLK | 450 | Ground

#### Left Roof Rail Reading Lamp

Connector Part Information |

• | 12047781

• | 3-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground
C | -- | -- | Not Used

#### Left Sunshade Lighted Vanity Mirror

Connector Part Information |

• | 12047663

• | 2-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground

#### Left Taillamp

Connector Part Information |

• | 12052848

• | 6-Way F Metri-Pack 150 Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 18 | Tail/turn/stoplamp feed - left rear
B | LT GRN/BLK | 24 | Backup lamp feed
C | -- | -- | Not Used
D | BRN | 9 | Park lamp feed
E | BLK | 350 | Ground
F | WHT | 17 | Stop lamp switch output

#### Left Window Switch

Connector Part Information |

• | 12064998

• | 8-Way F Metri-Pack 280 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 165 | Left front window motor feed-left front window-DOWN
B | LT BLU | 166 | Right front window switch feed-Right front window-UP
C | -- | -- | Not Used
D | GRY | 8 | Interior lamp dim signal
E | DK BLU | 164 | Power window motor feed-left front window-up direction
F | TAN | 167 | Left front window switch feed-Right front window DOWN
G | BLK | 750 | Ground
H | BRN | 141 | Fused ignition 3 feed

#### Liftgate Lock C1 (Door Ajar Switch)

Connector Part Information |

• | 12162190

• | 4-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 49 | Passenger door ajar switch signal
B | YEL | 804 | Door ajar indicator lamp output
C | -- | -- | Not Used
D | BLK | 450 | Ground

#### Rear Window Wiper/Washer and Multi-function Switch C1

Connector Part Information |

• | 12162502

• | 8-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | 1450 | Ground
2 | GRY | 8 | Interior lamp dim signal
3-4 | -- | -- | Not Used
5 | WHT | 393 | Rear window wiper motor feed
6 | GRY | 391 | Rear window wiper switch output
7 | -- | -- | Not Used
8 | DK GRN | 392 | Rear window washer pump motor feed

#### Rear Window Wiper/Washer and Multi-function Switch C2

Connector Part Information |

• | 12162455

• | 8-Way F Metri-Pack 280 Series (Natural)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 1176 | Auxiliary blower resistor output-low
B | ORN | 1052 | Auxiliary blower motor output
C | LT BLU | 1072 | Auxiliary blower resistor ouput-medium
D | -- | -- | Not Used
E | BLK | 1450 | Ground
F | -- | -- | Not Used
G | GRY | 778 | Auxiliary blower motor switch output
H | GRY | 8 | Interior lamp dim signal

#### Rear Window Wiper/Washer and Multi-function Switch C3

Connector Part Information |

• | 12041301

• | 8-Way F Metri-Pack 280 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior lamp dim signal
B | BLK | 1450 | Ground
C | BRN/WHT | 1571 | Traction control request input
D | BRN | 9 | Park lamp feed
E | YEL | 317 | Fog lamp relay feed-coil
F | PNK | 39 | Fused ignition 1 feed
G | PPL | 1681 | Traction control request received indicator lamp
H | PPL | 34 | Fog lamp feed

#### Relay Center

Connector Part Information |

• | 12160504

• | 36-Way F Metri-Pack Flexlock (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1-A9 | -- | -- | Not Used
B1 | ORN | 1640 | Fused battery feed
B2 | -- | -- | Not Used
B3 | ORN | 1640 | Fused battery feed
B4 | -- | -- | Not Used
B5 | PPL | 293 | Rear defogger element feed
B6 | -- | -- | Not Used
B7 | BRN | 241 | Fused ignition 3 feed
B8-B9 | -- | -- | Not Used
C1 | BRN/WHT | 301 | Theft deterrent relay output-coil-park lamp switch signal-parklamps ON
C2 | -- | -- | Not Used
C3 | BRN | 9 | Park lamp feed
C4 | -- | -- | Not Used
C5 | WHT | 193 | Rear defogger relay output-coil
C6 | -- | -- | Not Used
C7 | ORN | 1040 | Fused battery feed
C8-D9 | -- | -- | Not Used

#### Right Front Door Lock C1 (Ajar Indicator Switch)

Connector Part Information |

• | 12162190

• | 4-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 750 | Ground
B | -- | -- | Not Used
C | YEL | 804 | Door ajar indicator lamp output
D | DK BLU | 49 | Passenger door ajar switch signal

#### Right Front Door Lock Switch

Connector Part Information |

• | 12089527

• | 6-Way F Metri-Pack 280 Series (LT Green)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 195 | Door lock switch input-battery
B | BLK | 750 | Ground
C | GRY | 8 | Interior lamp dim signal
D | WHT | 194 | Door unlock switch input-battery
E | BLK | 750 | Ground
F | -- | -- | Not Used

#### Right Front Fog Lamp

Connector Part Information |

• | 12124819

• | 2-Way F Metri-Pack 280 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 34 | Fog lamp feed
B | BLK | 1250 | Ground

#### Right Front Park/Turn Lamp

Connector Part Information |

• | 12160394

• | Right Angle Type W-3 Bulb Base Sealed (Natural)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 15 | Turn signal lamp feed-right front
B | BRN | 9 | Park lamp feed
G | BLK | 1250 | Ground

#### Right Front Side Marker

Connector Part Information |

• | 12110053

• | Axial Type W-2 Bulb Base Sealed (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 19 | Tail/turn/stop lamp feed-right rear
B | BRN | 9 | Park lamp feed

#### Right Headlamp

Connector Part Information |

• | 12048369

• | 3-Way F Metri-Pack 280 Series Sealed (Blue)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1250 | Ground
B | TAN | 12 | Low beam headlamp feed
C | LT GRN | 11 | High beam headlamp feed

#### Right IP Courtesy Lamp

Connector Part Information |

• | 12124652

• | 2-Way Lamp Socket Wedge Base (Clear)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | GRY/BLK | 690 | Courtesy lights control output (GND)

#### Right License Lamp

Connector Part Information |

• | 12110053

• | Type W-2 F Axial Bulb Base (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Park lamp feed
B | BLK | 450 | Ground

#### Right Rear Door Latch Release Actuator Switch

Connector Part Information |

• | 12064860

• | 6-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 1894 | Power sliding door switch signal
B | GRY | 8 | Interior lamp dim signal
C | -- | -- | Not Used
D | BLK | 650 | Ground
E | BLK | 650 | Ground
F | -- | -- | Not Used

#### Right Rear Roof Rail Reading Lamp

Connector Part Information |

• | 12047781

• | 3-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground

#### Right Roof Rail Reading Lamp

Connector Part Information |

• | 12047781

• | 3-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground
C | -- | -- | Not Used

#### Right Sunshade Lighted Vanity Mirror

Connector Part Information |

• | 12047663

• | 2-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground

#### Right Taillamp

Connector Part Information |

• | 12052848

• | 6-Way F Metri-Pack 150 Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 19 | Tail/turn/stoplamp feed - right rear
B | LT GRN/BLK | 24 | Backup lamp feed
C | -- | -- | Not Used
D | BRN | 9 | Park lamp feed
E | BLK | 350 | Ground
F | WHT | 17 | Stop lamp switch output

#### Right Window Switch

Connector Part Information |

• | 12064998

• | 8-Way F Metri-Pack 280 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 666 | Power window motor feed-right front window-UP
B | GRY | 8 | Interior lamp dim signal
C | BLK | 750 | Ground
D | TAN | 167 | Left front window switch feed-Right front window-DOWN
E | BRN | 667 | Power window motor feed-right front window-DOWN
F | BRN | 141 | Fused ignition 3 feed
G | -- | -- | Not Used
H | LT BLU | 166 | Right front window switch feed-Right front window-UP

#### Stop Lamp Switch C1

Connector Part Information |

• | 12033701

• | 2-Way F Metri-Pack 480 Series (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 140 | Fused battery feed
B | WHT | 17 | Stop lamp switch output

#### Transaxle Range Switch C1

Connector Part Information |

• | 12129840

• | 7-Way F Metri-Pack Mixed Series Sealed (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 434 | PARK/NEUTRAL input
B | ORN | 840 | Fused battery feed
C | LT GRN | 275 | Transaxle range switch feed-PARK
D | BLK/WHT | 451 | PCM ground
E | PPL | 6 | Starter solenoid feed
F | LT GRN/BLK | 24 | Backup lamp feed
G | YEL | 5 | Ignition switched battery feed-START

#### Underhood Lamp

Connector Part Information |

• | 12052644

• | 2-Way F Metri-Pack 150 Series Sealed (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 1393 | Courtesy lamps feed-protected battery
B | BLK | 1250 | Ground

#### Windshield Header Courtesy/Reading Lamps

Connector Part Information |

• | 12047781

• | 3-Way F Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 328 | Interior lamp override switch output
B | BLK | 650 | Ground
C | GRY/BLK | 690 | Courtesy lights control output (GND)