For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Automatic Transaxle | Lower LH side of engine compartment | -- | --
Brake Transmission Shift Lock Control Actuator (BTSI) | Inside steering column near ignition switch | -- | --
Body Control Module (BCM) | Below RH side of I/P compartment | Body Control Module Component Views | Body Control Module Connector End Views
Fuse Block | RH side of I/P,in RH front door opening | Power and Grounding Component Views | --
Ignition Switch | Inside steering column | -- | --
LH Tail Lamp | Rear of vehicle, LH side | -- | --
Powertrain Control Module (PCM) | Engine compartment, inside air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Rear Side Door Actuator Motor | RH quarter panel, above wheelhouse | -- | --
RH Tail Lamp | Rear of vehicle, RH side | -- | --
Starter Solenoid | Lower front of engine, part of starter motor assembly | -- | --
Stop Lamp Switch | Mounted to brake pedal support | Antilock Brake System Component Views | Cruise Control Connector End Views
Transaxle Range Switch | Rear LH side of engine compartment, mounted to top of transaxle | Automatic Transmission Electronic Component Views | Engine Controls Connector End Views
Underhood Accessory Wiring Junction Block 1 | Engine compartment, front of RH wheelhouse, above battery | Power and Grounding Component Views | Power and Grounding Connector End Views
Underhood Accessory Wiring Junction Block 2 | Engine compartment, front of RH wheelhouse, above battery | Power and Grounding Component Views | Power and Grounding Connector End Views
Vehicle Speed Sensor (VSS) | Lower RR of engine compartment , on transaxle | -- | --
C103 (2 cavities) | I/P wiring harness to engine wiring harness , LH side of engine compartment, next to C101 and C181 | Harness Routing Views | Inline Harness Connector End Views
C111 (7 cavities) | Engine harness to automatic transaxle harness, LH side of engine compartment, top of transmission | Harness Routing Views | Inline Harness Connector End Views
C201 (48 cavities) | I/P wiring harness to steering column wiring harness, mounted to LH side of steering column near base | Harness Routing Views | Inline Harness Connector End Views
G113 | Engine compartment, left of starter, along with battery ground | Harness Routing Views | --
G402 | Secured to lower RH D-piller | -- | --
P100 | On RH side of bulkhead, left of RH strut tower | Harness Routing Views | --
P400 | Behind RH taillamp | Harness Routing Views | --
P401 | Behind LH taillamp | Harness Routing Views | --
S106 | Engine harness, front LH side of engine compartment approximately 10 cm (4 in) from PCM breakout | -- | --
S122 | Engine harness, on RH side of engine compartment approximately 15 cm (6 in) from PCM breakout | -- | --
S209 | I/P harness, center of I/P approximately 8 cm (3 in) from security indicator lamp breakout | -- | --
S406 | Body harness, LR of body approximately 17 cm (7 in) from P401 breakout | -- | --