For 1990-2009 cars

#### Front Suspension

(1) | Front Stabilizer Shaft Insulator Clamp Bolt
(2) | Front Stabilizer Shaft Link Nut
(3) | Front Suspension Strut Mount Nut
(4) | Front Suspension Spring
(5) | Front Suspension Strut
(6) | Strut to Knuckle Nut
(7) | Front Steering Knuckle
(8) | Strut to Knuckle Bolt
(9) | Front Stabilizer Shaft Link
(10) | Front Lower Control Arm
(11) | Front Lower Control Arm Bolt
(12) | Front Lower Control Arm Nut
(13) | Frame
(14) | Front Stabilizer Shaft Insulator
(15) | Front Stabilizer Shaft
(16) | Front Stabilizer Shaft Clamp

The replacement of any of the following items does not require the inspection or adjustment of the camber or the toe:

• | The strut bumper

• | The strut shield

• | The upper spring seat

• | The strut bearing

• | The spring insulators

If you replace any of the following components, inspect and adjust the camber and the toe:

• | The strut damper

• | The knuckle

• | The control arm

• | The strut mount

• | The spring