For 1990-2009 cars

#### In-line Connector C101

Connector Part Information |

• | 12065426

• | 10-Way F Micro-Pack 150 Series Sealed (Gray)

Connector Part Information

• | 12052189

• | 10-Way M Micro-Pack 150 Series Sealed (Gray)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PPL | 1807 | Class 2 Serial Data Communication | A | PPL | 1807 | Class 2 Serial Data Communication
B | TAN | 800 | UART Serial Data Communication | B | TAN | 800 | UART Serial Data Communication
C | ORN/BLK | 463 | Desired Torque | C | ORN/BLK | 463 | Desired Torque
D | TAN/BLK | 464 | Delivered Torque | D | TAN/BLK | 464 | Delivered Torque
E | DK GRN/WHT | 762 | A/C Request Signal | E | DK GRN/WHT | 762 | A/C Request Signal
F | -- | -- | Not Used | F | -- | -- | Not Used
G | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | G | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
H | WHT | 1310 | Canister Vent Valve Solenoid Output | H | WHT | 1310 | Canister Vent Valve Solenoid Output
J | -- | -- | Not Used | J | -- | -- | Not Used
K | DK BLU | 229 | Theft Deterrent Fuel Enable Signal | K | DK BLU | 229 | Theft Deterrent Fuel Enable Signal

#### In-line Connector C102

Connector Part Information |

• | 12065425

• | 10-Way F Metri-Pack 150 Series Sealed (Black)

Connector Part Information

• | 12048253

• | 10-Way M Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 1744 | Fuel Injector 1 Control | A | BLK | 1744f | Fuel Injector 1 Control
B | LT GRN/BLK | 1745 | Fuel Injector 2 Control | B | LT GRN/BLK | 1745 | Fuel Injector 2 Control
C | PNK/BLK | 1746 | Fuel Injector 3 Control | C | PNK/BLK | 1746 | Fuel Injector 3 Control
D | PNK | 639 | Fused Ignition 1 Feed | D | PNK | 639 | Fused Ignition 1 Feed
E | ORN/BLK | 469 | PCM Sensor Ground | E | ORN/BLK | 469 | MAP Sensor Return
F | GRY | 416 | 5 Volt Reference Signal | F | GRY | 416 | 5 Volt Reference Signal
G | LT GRN | 432 | MAP Sensor Signal | G | LT GRN | 432 | MAP Sensor Signal
H | YEL/BLK | 846 | Fuel Injector 6 Control | H | YEL/BLK | 846 | Fuel Injector 6 Control
J | BLK/WHT | 845 | Fuel Injector 5 Control | J | BLK/WHT | 845 | Fuel Injector 5 Control
K | LT BLU/BLK | 844 | Fuel Injector 4 Control | K | LT BLU/BLK | 844 | Fuel Injector 4 Control

#### In-line Connector C103

Connector Part Information |

• | 12052613

• | 2-Way F Metri-Pack 480 Series Sealed (Black)

Connector Part Information

• | 12065863

• | 2-Way M Metri-Pack 480 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 5 | Ignition Switched Battery Feed-START | A | YEL | 5 | Ignition Switched Battery Feed-START
B | RED | 102 | Fusible Link Battery Feed to ABS Relay | B | RED | 102 | Fusible Link Battery Feed to ABS Relay

#### In-line Connector C105

Connector Part Information |

• | 12052613

• | 2-Way F Metri-Pack 480 Series Sealed (Black)

Connector Part Information

• | 12186012

• | 2-Way M Metri-Pack 480 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 504 | Engine Coolant Fan 2 (Left) Feed | A | WHT | 504 | Engine Coolant Fan 2 (Left) Feed
B | BLK | 532 | Ground | B | BLK | 532 | Ground

#### In-line Connector C108

Connector Part Information |

• | 12110293

• | 3-Way F Metri-Pack 150 Series Sealed (Black)

Connector Part Information

• | 12129615

• | 3-Way M Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 2761 | PCM Sensor Ground | A | BLK | 2761 | PCM Sensor Ground
B | YEL | 410 | Engine Coolant Temperature Sensor Signal | B | YEL | 410 | Engine Coolant Temperature Sensor Signal
C | DK GRN | 135 | Engine Coolant Temperature Sensor | C | DK GRN | 135 | Engine Coolant Temperature Sensor

#### In-line Connector C111

Connector Part Information |

• | 12129508

• | 7-Way F Metri-Pack 150 (Black)

Connector Part Information

• | 12146356

• | 7-Way F Metri-Pack 150 (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 1222 | 1-2 Shift Solenoid Valve Control | A | LT GRN | 1222 | 1-2 Shift Solenoid Valve Control
B | YEL/BLK | 1223 | 2-3 Shift Solenoid Valve Control | B | YEL | 1223 | 2-3 Shift Solenoid Valve Control
C | BRN | 418 | TCC PWM SOL Valve Control | C | BLK | 418 | TCC PWM SOL Valve Control
D | TAN/BLK | 422 | TCC SOL valve control | D | TAN | 422 | TCC SOL valve control
E | PNK | 1339 | Fused Ignition 1 Feed | E | RED | 1339 | Fused Ignition 1 Feed
F | YEL/BLK | 1227 | Transmission Fluid Temperature Sensor Signal | F | BRN | 1227 | Transmission Fluid Temperature Sensor Signal
G | ORN/BLK | 1057 | PCM Sensor Ground | G | GRY | 1057 | PCM Sensor Ground

#### In-line Connector C120

Connector Part Information |

• | 12110293

• | 3-Way F Metri-Pack 150 Series Sealed (Black)

Connector Part Information

• | 12129615

• | 3-Way M Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN/BLK | 735 | Ambient Air Temperature Sensor Signal | A | LT GRN/BLK | 735 | Ambient Air Temperature Sensor Signal
B | BLK | 1550 | Ground | B | BLK | 1550 | Ground
C | DK BLU | 1393 | Courtesy Lamps Feed-Protected Battery | C | DK BLU | 1393 | Courtesy Lamps Feed-Protected Battery

#### In-line Connector C171

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series (Black)

Connector Part Information

• | 12162000

• | 2-Way M Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 830 | Left Front Wheel Speed Signal-High | A | LT BLU | 830 | Left Front Wheel Speed Signal-High
B | WHT | 873 | Left Front Wheel Speed Signal-Low | B | YEL | 873 | Left Front Wheel Speed Sensor-Low

#### In-line Connector C172

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series (Black)

Connector Part Information

• | 12162000

• | 2-Way M Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 833 | Right Front Wheel Speed Signal-Low | A | TAN | 833 | Right Front Wheel Speed Signal-Low
B | BLK | 872 | Right Front Wheel Speed Signal-High | B | DK GRN | 872 | Right Front Wheel Speed Signal-High

#### In-line Connector C181

Connector Part Information |

• | 12052848

• | 6-Way F Metri-Pack 150 Series (Black)

Connector Part Information

• | 12124107

• | 6-Way M Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN/BLK | 1057 | PCM Sensor Ground | A | ORN/BLK | 1057 | PCM Sensor Ground
B | ORN/BLK | 434 | PARK/NEUTRAL Input | B | ORN/BLK | 434 | PARK NEUTRAL Input
C | PPL | 1589 | Fuel Level Sensor Input | C | PPL | 1589 | Fuel Level Sensor Input
D | ORN | 55 | Fuel Level Gauge Sensor Signal | D | ORN | 55 | Fuel Level Gauge Sensor Signal
E | GRY | 474 | 5-Volt Reference | E | GRY | 474 | 5-Volt Reference
F | -- | -- | Not Used | F | -- | -- | Not Used

#### In-line Connector C200

Connector Part Information |

• | 12034257

• | 56-Way F Metri-Pack Mixed Series (Black)

Connector Part Information

• | 12186339

• | 56-Way M Metri-Pack Mixed Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | ORN | 340 | Fused Battery Feed | A1 | ORN | 340 | Fused Battery Feed
A2 | LT BLU | 1894 | Power Sliding Door Switch Signal | A2 | LT BLU | 1894 | Power Sliding Door Switch Signal
A3-A6 | -- | -- | Not Used | A3-A6 | -- | -- | Not Used
A7 | GRY | 120 | Fuel Pump Motor Feed | A7 | GRY | 120 | Fuel Pump Motor Feed
A8 | BRN | 141 | Fused Ignition 3 Feed | A8 | BRN | 141 | Fused Ignition 3 Feed
A9 | BRN | 541 | Fused Ignition 3 Feed | A9 | BRN/WHT | 541 | Fused Ignition 3 Feed
B1 | PNK | 839 | Not Used | B1 | -- | -- | Not Used
B2 | LT GRN | 275 | Transaxle Range Switch Feed-PARK | B2 | LT GRN | 275 | Transaxle Range Switch Feed-PARK
B3 | GRY/BLK | 690 | Courtesy Lamp Control | B3 | GRY/BLK | 690 | Courtesy Lamp Control
B4 | ORN | 1240 | Fused Battery Feed | B4 | ORN | 1240 | Fused Battey Feed
B6-B7 | -- | -- | Not Used | B6-B7 | -- | -- | Not Used
B8 | DK BLU | 1393 | Courtesy Lamps Feed-Protected Battery | B8 | DK BLU | 1393 | Courtesy Lamps Feed-Protected Battery
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used
C1 | PPL | 328 | Interior Lamp Override Switch Output | C1 | PPL | 328 | Interior Lamp Override Switch Output
C2 | YEL | 1139 | Fused Ignition 1 Feed | C2 | YEL | 1139 | Fused Ignition 1 Feed
C3 | BRN | 358 | Airbag Indicator Lamp Output | C3 | BRN | 358 | Airbag Indicator Lamp Output
C4 | -- | -- | Not Used | C4 | -- | -- | Not Used
C6 | LT GRN/BLK | 735 | Ambient Air Temperature Sensor Signal | C6 | LT GRN/BLK | 735 | Ambient Air Temperature Sensor Signal
C7 | DK GRN | 389 | Vehicle Speed Signal (VSS) | C7 | DK GRN | 389 | Vehicle Speed Signal (VSS)
C8 | -- | -- | Not Used | C8 | -- | -- | Not Used
C9 | PNK | 1039 | Fused Igniton 1 Feed | C9 | PNK | 1039 | Fused Ignition 1 Feed
D1-D2 | -- | -- | Not Used | D1-D2 | -- | -- | Not Used
D3 | BRN | 741 | Fused Ignition 3 Feed | D3 | BRN | 741 | Fused Ignition 3 Feed
D6 | ORN | 1140 | Fused Battery Feed | D6 | ORN | 1140 | Fused Battery Feed
D7-D8 | -- | -- | Not Used | D7-D8 | -- | -- | Not Used
E1 | -- | -- | Not Used | E1 | -- | -- | Not Used
E2 | TAN | 159 | LF Door Ajar Indicator | E2 | TAN | 159 | LF Door Ajar Indicator
E3 | DK BLU | 49 | Passenger Door Ajar Switch Signal | E3 | DK BLU | 49 | Passenger Door Ajar Switch Signal
E4-E6 | -- | -- | Not Used | E4-E6 | -- | -- | Not Used
E7 | BLK/WHT | 238 | Seat Belt Switch Input | E7 | BLK/WHT | 238 | Seat Belt Switch Input
E8-E9 | -- | -- | Not Used | E8-E9 | -- | -- | Not Used
F1 | TAN | 294 | Passenger Door Lock Motor Feed-Unlock | F1 | TAN | 294 | Passenger Door Lock Motor Feed-Unlock
F2 | GRY | 295 | Passenger Door Lock Motor Feed-Lock | F2 | GRY | 295 | Passenger Door Lock Motor Feed-Lock
F3 | ORN | 54 | Sliding Door Ajar Signal Battery | F3 | BLK | 54 | Sliding Door Ajar Signal Battery
F4 | -- | -- | Not Used | F4 | -- | -- | Not Used
F6 | ORN | 2540 | Fused Battery Feed | F6 | ORN | 2540 | Fused Battery Feed
F7 | PPL | 293 | Rear Defogger Element Feed | F7 | PPL | 293 | Rear Defogger Element Feed
F8-F9 | -- | -- | Not Used | F8-F9 | -- | -- | Not Used
G1 | -- | -- | Not Used | G1 | -- | -- | Not Used
G2 | LT BLU | 195 | Door Lock Switch Input-Battery | G2 | LT BLU | 195 | Door Lock Switch Input Battery
G3 | RED/BLK | 780 | Door Lock-Key Cylinder | G3 | RED/BLK | 780 | Door Lock-Key Cylinder
G4 | ORN/BLK | 781 | Door Unlock-Key Cylinder | G4 | ORN/BLK | 781 | Door Unlock-Key Cylinder
G5 | -- | -- | Not Used | G5 | -- | -- | Not Used
G6 | TAN | 694 | Driver Door Unlock-Battery | G6 | TAN | 694 | Driver Door Unlock-Battery
G7 | WHT | 194 | Door Unlock Switch Input-Battery | G7 | WHT | 194 | Door Unlock Switch Input-Battery
G8-G10 | -- | -- | Not Used | G8-G10 | -- | -- | Not Used

#### In-line Connector C201

Connector Part Information |

• | 12047842

• | 17-Way F Metri-Pack 150 Series (Black)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | -- | -- | Not Used | A1 | -- | -- | Not Used
A2 | PNK | 539 | Fused Ignition 1 Feed | A2 | PND | 539 | Fused Ignition 1 Feed
A3 | -- | -- | Not Used | A3 | -- | -- | Not Used
A4 | PPL | 16 | Turn Signal Flasher Output | A4 | PPL | 16 | Turn Signal Flasher Output
A5 | -- | -- | Not Used | A5 | -- | -- | Not Used
A6 | DK BLU | 1415 | Turn Signal Lamp Feed-Right Front | A6 | DK BLU/WHT | 1415 | Turn Signal Lamp Feed-Right Front
A7 | LT BLU | 1414 | Turn Signal Lamp Feed-Left Front | A7 | LT BLU/WHT | 1414 | Turn Signal Lamp Feed-Left Front
A8-A10 | -- | -- | Not Used | A8-A10 | -- | -- | Not Used
A11 | BLK | 28 | Horn Relay Output-Coil | A11 | BLK | 28 | Horn Relay Output-Coil
A12 | GRY | 397 | Cruise ON/OFF Signal | A12 | GRY | 397 | Cruise ON/OFF Signal
A13 | PNK | 739 | Fused Ignition 1 Feed | A13 | PNK | 739 | Fused Ignition 1 Feed
A14 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal | A14 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal
A15 | GRY/BLK | 87 | Cruise Control RESUME/ACCELERATE Switch Signal | A15 | GRY/BLK | 87 | Cruise Control RESUME/ACCELERATE Switch Signal
A16 | BLK | 434 | PARK/NEUTRAL Input | A16 | ORN/BLK | 434 | PARK/NEUTRAL Input
A17 | DK GRN/WHT | 1135 | Stop Lamp Switched BTSI Feed | A17 | DK GRN/WHT | 1135 | Stop Lamp Switched BTSI Feed

#### In-line Connector C201

Connector Part Information |

• | 12084183

• | 18-Way F Metri-Pack Mixed Series (Black)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
B1 | -- | -- | Not Used | B1 | -- | -- | Not Used
B2 | BLK | 150 | Ground | B2 | BLK | 150 | Ground
B3 | LT GRN | 80 | Key In Ignition Input | B3 | LT GRN | 80 | Key In Ignition Input
B4 | TAN/WHT | 1559 | Ground | B4 | BLK | 1550 | Ground
B5-B6 | -- | -- | Not Used | B5-B6 | -- | -- | Not Used
C1 | WHT | 1390 | Ignition Switched Battery Feed-Ignition 0 | C1 | WHT | 1390 | Ignition Switched Battery Feed-Ignition 0
C2 | BLK | 150 | Ground | C2 | BLK | 150 | Ground
C3-C4 | -- | -- | Not Used | C3C4 | -- | -- | Not Used
C5 | PNK | 3 | Ignition Switched Battery Feed-Ignition 1 | C5 | PNK | 3 | Ignition Switched Battery Feed-Ignition 1
C6 | ORN | 300 | Ignition Switched Battery Feed-Ignition 3 | C6 | ORN | 300 | Ignition Switched Battery Feed-Ignition 3
D1 | YEL | 5 | Ignition Switched Battery Feed-START | D1 | YEL | 5 | Ignition Switched Battery Feed-START
D2 | RED | 142 | Fused Battery Feed | D2 | RED | 142 | Fused Battery Feed
D3-D4 | -- | -- | Not Used | D3-D4 | -- | -- | Not Used
D5 | RED | 42 | Fused Battery Feed | D5 | RED | 42 | Fused Battery Feed
D6 | BRN | 4 | Ignition Switched Battery Feed-Accessory | D6 | BRN | 4 | Ignition Switched Battery Feed-Accessory

#### In-line Connector C201

Connector Part Information |

• | 12047840

• | 13-Way F Metri-Pack 280 Series (LT Gray)

Connector Part Information

• | 12077822

• | 48-Way M Metri-Pack Mixed Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
E1 | LT BLU | 1508 | Turn Signal Lamp/Hazard Lamp Flasher Feed | E1 | LT BLU | 1508 | Turn Signal Lamp/Hazard Lamp Flasher Feed
E2 | DK GRN | 113 | Windshield Wiper Switch Signal-ON | E2 | DK GRN | 113 | Windshield Wiper Switch Signal-ON
E3 | GRY | 112 | Windshield Wiper Switch Signal-LOW/PULSE | E3 | GRY | 112 | Windshield Wiper Switch Signal-LOW/PULSE
E4 | PPL | 92 | Windshield Wiper Motor Feed-High Speed | E4 | PPL | 92 | Windshield Wiper Motor
E5 | RED | 229 | Windshield Washer Pump Motor Feed | E5 | RED | 228 | Windshield Washer Pump Motor Feed
E6 | DK GRN | 19 | Tail/Turn Stop Lamp Feed-Right Rear | E6 | DK GRN | 19 | Tail/Turn Stop Lamp Feed-Right Rear
E7 | YEL | 18 | Tail/Turn Stop Lamp Feed-Left Rear | E7 | YEL | 18 | Tail/Turn Stop Lamp Feed-Left Rear
E8 | ORN | 1840 | Fused Battery Feed | E8 | ORN | 1840 | Fused Battery Feed
E9 | YEL/BLK | 243 | Fused Accessory Feed | E9 | YEL | 243 | Fused Accessory Feed
E10 | YEL/BLK | 2340 | Fused Battery Feed | E10 | ORN | 2340 | Fused Battery Feed
E11 | LT GRN | 11 | High Beam Headlamp Feed | E11 | LT GRN | 11 | High Beam Headlamp Feed
E12 | TAN | 12 | Low Beam Headlamp Feed | E12 | TAN | 12 | Low Beam Headlamp Feed
E13 | YEL | 10 | Headlamp Switch Output | E13 | YEL | 10 | Headlamp Switch Output

#### In-line Connector C203

Connector Part Information |

• | 12034257

• | 56-Way F Metri-Pack Mixed Series (Black)

Connector Part Information

• | 12186339

• | 56-Way M Metri-Pack Mixed Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | ORN | 1052 | Auxiliary Blower Motor Output | A1 | ORN | 1052 | Auxiliary Blower Motor Output
A2 | YEL | 18 | Tail/Turn/Stop Lamp Feed-Left Rear | A2 | YEL | 18 | Tail/Turn/Stop Lamp Feed-Left Rear
A3 | DK GRN | 19 | Tail/Turn/Stop Lamp Feed-Right Rear | A3 | DK GRN | 19 | Tail/Turn/Stop Lamp Feed-Right Rear
A4 | LT BLU | 1134 | Park Brake Switch Signal | A4 | LT BLU | 1134 | Park Brake Switch Signal
A6 | -- | -- | Not Used | A6 | -- | -- | Not Used
A7 | GRY | 778 | Auxiliary Blower Motor Switch Output | A7 | GRY | 778 | Auxiliary Blower Motor Switch Output
A8 | WHT | 17 | Stop Lamp Switch Output | A8 | WHT | 17 | Stop Lamp Switch Output
A9 | YEL | 43 | Fused Accessory Feed | A9 | YEL | 43 | Fused Accessory Feed
B1 | -- | -- | Not Used | B1 | -- | -- | Not Used
B2 | GRY | 391 | Rear Window Wiper Switch Output | B2 | GRY | 391 | Rear Window Wiper Switch Output
B3 | BRN | 882 | Right Rear Wheel Speed Signal-High | B3 | BRN | 882 | Right Rear Wheel Speed Signal-High
B4 | WHT | 883 | Right Rear Wheel Speed Signal-Low | B4 | WHT | 883 | Right Rear Wheel Speed Signal-Low
B6 | BRN | 9 | Park Lamp Feed | B6 | BRN | 9 | Park Lamp Feed
B7 | WHT | 393 | Rear Window Wiper Motor Feed | B7 | WHT | 393 | Rear Window Wiper Motor Feed
B8 | DK GRN | 392 | Rear Window Washer Pump Motor Feed | B8 | DK GRN | 392 | Rear Window Washer Pump Motor Feed
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used
C1 | BLK | 884 | Left Rear Wheel Speed Signal-High | C1 | BLK | 884 | Left Rear Wheel Speed Signal-High
C2 | RED | 885 | Left Rear Wheel Speed Signal-Low | C2 | RED | 885 | Left Rear Wheel Speed Signal-Low
C3 | LT BLU | 733 | Temperature Valve Position Signal | C3 | LT BLU | 733 | Temperature Valve Position Signal
C4 | -- | -- | Not Used | C4 | -- | -- | Not Used
C6 | YEL | 804 | Door Ajar Indicator Lamp Output | C6 | YEL | 804 | Door Ajar Indicator Lamp Output
C7 | TAN | 800 | UART Serial Data Communication | C7 | TAN | 800 | UART Serial Data Communication
C8 | PPL | 1589 | Fuel Level Sensor Input | C8 | PPL | 1589 | Fuel Level Sensor Input
C9 | -- | -- | Not Used | C9 | -- | -- | Not Used
D1 | LT BLU | 1072 | Auxiliary Blower Resistor Output-Medium | D1 | LT BLU | 1072 | Auxiliary Blower Resistor Output Medium
D2 | BLK/WHT | 351 | Ground-Clean | D2 | BLK/WHT | 351 | Ground-Clean
D3 | GRY | 8 | Interior Lamp Dim Signal | D3 | GRY | 8 | Interior Lamp Dim Signal
D6 | -- | -- | Not Used | D6 | -- | -- | Not Used
D7 | ORN/BLK | 1057 | PCM Sensor Ground | D7 | ORN/BLK | 1057 | PCM Sensor Ground
D8 | ORN | 640 | Fused Battery Feed | D8 | ORN | 640 | Fused Battery Feed
E1 | DK BLU | 46 | Speaker Feed-Right Rear | E1 | DK BLU | 46 | Speaker Feed-Right Rear
E2 | TAN | 201 | Speaker Feed-Left Front | E2 | TAN | 201 | Speaker Feed-Left Front
E3 | LT GRN | 200 | Speaker Feed-Right Front | E3 | LT GRN | 200 | Speaker Feed-Right Front
E4 | YEL | 116 | Speaker Return-Left Rear | E4 | YEL | 116 | Speaker Return-Left Rear
E6 | GRY | 474 | 5-Volt Reference | E6 | GRY | 474 | 5-Volt Reference
E7 | BLK | 906 | RSA Enable Out | E7 | BLK | 906 | RSA Enable Out
E8 | LT GRN | 1011 | RSA Enable In | E8 | LT GRN | 1011 | RSA Enable In
E9 | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | E9 | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
F1 | GRY/BLK | 308 | Park Lamp Switch Output-Parklamps ON | F1 | GRY/BLK | 308 | Park Lamp Switch Output-Parklamps ON
F2-F4 | -- | -- | Not Used | F2-F4 | -- | -- | Not Used
F6 | YEL | 1176 | Auxiliary Blower Resistor Output-Low | F6 | YEL | 1176 | Auxiliary Blower Resistor Output-Low
F7 | LT GRN/BLK | 24 | Backup Lamp Feed | F7 | BLK | 24 | Backup Lamp Feed
F8 | BLK | 1550 | Ground | F8 | BLK | 1550 | Ground
F9 | -- | -- | Not Used | F9 | -- | -- | Not Used
G1 | -- | -- | Not Used | G1 | -- | -- | Not Used
G2 | BRN | 641 | Fused Ignition 3 Feed | G2 | BRN | 641 | Fused Ignition 3 Feed
G3 | PNK | 39 | Fused Ignition 1 Feed | G3 | PNK | 39 | Fused Ignition 1 Feed
G4 | WHT | 1310 | Canister Vent Valve Solenoid Output | G4 | WHT | 1310 | Canister Vent Valve Solenoid Output
G5-G6 | -- | -- | Not Used | G5-G6 | -- | -- | Not Used
G7 | BRN | 199 | Speaker Feed-Left Rear | G7 | BRN | 199 | Speaker Feed-Left Rear
G8 | LT BLU | 115 | Speaker Return-Right Rear | G8 | LT BLU | 115 | Speaker Return-Right Rear
G9 | DK GRN | 117 | Speaker Return-Right Front | G9 | DK GRN | 117 | Speaker Return-Right Front
G10 | GRY | 118 | Speaker Return-Left Front | G10 | GRY | 118 | Speaker Return-Left Front

#### In-line Connector C205

Connector Part Information |

• | 12092162

• | 4-Way F Metri-Pack 280 Series Sealed (Gray)

Connector Part Information

• | 12162477

• | 4-Way M Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 443 | Fused accessory feed | A | YEL | 443 | Fused accessory feed
B | BRN | 1244 | Fused I/P dim signal | B | BRN | 1244 | Fused I/P dim signal
C | LT GRN | 1796 | Radio control signal-steering column | C | DK BLU | 1796 | Radio control signal-steering column
D | BLK/WHT | 1450 | Ground | D | BLK | 1450 | Ground

#### In-line Connector C215

Connector Part Information |

• | 12092865

• | 2-Way F Metri-Pack 280 Series (Yellow)

Connector Part Information

• | 12110149

• | 2-Way M Metri-Pack 280 Series (Yellow)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 347 | SIR inflator feed-driver | A | WHT | 347 | SIR inflator feed-driver
B | DK GRN | 348 | SIR inflator output-driver | B | DK GRN | 348 | SIR inflator output-driver

#### In-line Connector C216

Connector Part Information |

• | 12077921

• | 2-Way F Metri-Pack 280 Series (Yellow)

Connector Part Information

• | 12110288

• | 2-Way M Metri-Pack 280 Series (Yellow)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT/BLK | 1403 | Passenger inflator-high | A | WHT/BLK | 1403 | Passenger inflator-high
B | DK GRN/WHT | 1404 | Passenger inflator-low | B | DK GRN/WHT | 1404 | Passenger inflator-low

#### In-line Connector C301

Connector Part Information |

• | 12064769

• | 10-Way F Metri-Pack 150 Series (Natural)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (Natural)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 194 | Door unlock switch input-battery | A | WHT | 194 | Door unlock switch input-battery
B | TAN | 694 | Driver door unlock-battery | B | TAN | 694 | Driver door unlock-battery
C | LT BLU | 195 | Door lock switch input-battery | C | LT BLU | 195 | Door lock switch input-battery
D-K | -- | -- | Not Used | D-K | -- | -- | Not Used

#### In-line Connector C302

Connector Part Information |

• | 12129430

• | 16-Way F ACT 280 Series (White)

Connector Part Information

• | 12129429

• | 16-Way M ACT 280 Series (White)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 750 | Ground | A | BLK | 750 | Ground
B | DK GRN | 117 | Speaker feed-right front | B | DK GRN | 117 | Speaker feed-right front
C | LT GRN | 200 | Speaker return-right front | C | LT GRN | 200 | Speaker return-right front
D | -- | -- | Not Used | D | -- | -- | Not Used
E | BRN | 141 | Fused ignition 3 feed | E | BRN | 141 | Fused ignition 3 feed
F | LT BLU | 166 | Left front window switch feed-Right front window UP | F | LT BLU | 166 | Left front window switch feed-Right front window UP
G | DK BLU | 49 | Passenger door ajar switch signal | G | DK BLU | 49 | Passenger door ajar switch signal
H | YEL | 804 | Door ajar indicator lamp output | H | YEL | 804 | Door ajar indicator lamp output
J | GRY | 8 | Interior lamp dim signal | J | GRY | 8 | Interior lamp dim signal
K | TAN | 167 | Left front window switch feed-Right front window DOWN | K | TAN | 167 | Left front window switch feed-Right front window DOWN
L | RED/BLK | 780 | Door lock-key cylinder | L | RED/BLK | 780 | Door lock-key cylinder
M | ORN/BLK | 781 | Door unlock-key cylinder | M | ORN/BLK | 781 | Door unlock-key cylinder
N | RED/WHT | 881 | Right outside rearview mirror right/left feed | N | RED/WHT | 881 | Right outside rearview mirror right/left feed
P | LT BLU/WHT | 1497 | Right outside rearview mirror motor pack common feed | P | LT BLU/WHT | 1497 | Right outside rearview mirror motor pack common feed
R | BRN/WHT | 1498 | Right outside rearview mirror UP/DOWN feed | R | BRN/WHT | 1498 | Right outside rearview mirror UP/DOWN feed
S | GRY | 295 | Passenger door lock motor feed-lock | S | GRY | 295 | Passenger door lock motor feed-lock

#### In-line Connector C303

Connector Part Information |

• | 12129430

• | 16-Way F ACT 280 Series (White)

Connector Part Information

• | 12129429

• | 16-Way M ACT 280 Series (White)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 750 | Ground | A | BLK | 750 | Ground
B | GRY | 118 | Speaker feed-left front | B | GRY | 118 | Speaker feed-left front
C | TAN | 201 | Speaker return-left front | C | TAN | 201 | Speaker return-left front
D | ORN | 1140 | Fused battery feed | D | ORN | 1140 | Fused battery feed
E | BRN | 141 | Fused ignition 3 feed | E | BRN | 141 | Fused ignition 3 feed
F | LT BLU | 166 | Left front window switch feed-Right front window UP | F | LT BLU | 166 | Left front window switch feed-Right front window UP
G | TAN | 159 | Left front door ajar indicator | G | TAN | 159 | Left front door ajar indicator
H | YEL | 804 | Door ajar indicator lamp output | H | YEL | 804 | Door ajar indicator lamp output
J | GRY | 8 | Interior lamp dim signal | J | GRY | 8 | Interior lamp dim signal
K | TAN | 167 | Left front window switch feed-Right front window DOWN | K | TAN | 167 | Left front window switch feed-Right front window DOWN
L | RED/BLK | 780 | Door lock-key cylinder | L | RED/BLK | 780 | Door lock-key cylinder
M | ORN/BLK | 781 | Door unlock-key cylinder | M | ORN/BLK | 781 | Door unlock-key cylinder
N | RED/WHT | 881 | Right outside rearview mirror right/left feed | N | RED/WHT | 881 | Right outside rearview mirror right/left feed
P | LT BLU/WHT | 1497 | Right outside rearview mirror motor pack common feed | P | LT BLU/WHT | 1497 | Right outside rearview mirror motor pack common feed
R | BRN/WHT | 1498 | Right outside rearview mirror UP/DOWN feed | R | BRN/WHT | 1498 | Right outside rearview mirror UP/DOWN feed
S | GRY | 295 | Passenger door lock motor feed-lock | S | GRY | 295 | Passenger door lock motor feed-lock

#### In-line Connector C304

Connector Part Information |

• | 12064769

• | 10-Way F Metri-Pack 150 Series (Natural)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (Natural)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 194 | Door unlock switch input-battery | A | WHT | 194 | Door unlock switch input-battery
B | TAN | 294 | Passenger door lock motor feed-unlock | B | TAN | 294 | Passenger door lock motor feed-unlock
C | LT BLU | 195 | Door lock switch input-battery | C | LT BLU | 195 | Door lock switch input-battery
D-K | -- | -- | Not Used | D-K | -- | -- | Not Used

#### In-line Connector C305

Connector Part Information |

• | 12146439

• | 4-Way F Metri-Pack 150 Series Sealed (Gray)

Connector Part Information

• | 15317612

• | 12-Way M Metri-Pack 280 Series Sealed (Gray)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1A | BRN | 882 | Right rear wheel speed signal-high | 1A | BRN | 882 | Right rear wheel speed signal-high
1B | WHT | 883 | Right rear wheel speed signal-low | 1B | WHT | 883 | Right rear wheel speed signal-low
1C | BLK | 884 | Left rear wheel speed signal-high | 1C | BLK | 884 | Left rear wheel speed signal-high
1D | RED | 885 | Left rear wheel speed signal-low | 1D | RED | 885 | Left rear wheel speed signal-low

#### In-line Connector C305

Connector Part Information |

• | 12176335

• | 8-Way F Metri-Pack 280 Flexlock Series Sealed (Natural)

Connector Part Information

• | 15317612

• | 12-Way M Metri-Pack Mixed Series (Gray)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
3A | BLK | 250 | Ground | 3A | BLK | 250 | Ground
3B | BLK/WHT | 1057 | Ground-clean | 3B | ORN/BLK | 1057 | Ground-clean
3C | GRY | 120 | Fuel pump motor feed | 3C | GRY | 120 | Fuel pump motor feed
3D | PPL | 1589 | Fuel level sensor input | 3D | PPL | 1589 | Fuel level sensor input
3E | DK GRN | 890 | Fuel tank pressure sensor signal | 3E | DK GRN | 890 | Fuel tank pressure sensor signal
3F | WHT | 1310 | Canister vent valve solenoid output | 3F | WHT | 1310 | Canister vent valve solenoid output
3G | PNK | 1039 | Fused ignition 1 feed | 3G | PNK | 1039 | Fused ignition 1 feed
3H | GRY/BLK | 474 | 5-volt reference | 3H | GRY/BLK | 474 | 5-volt reference

#### In-line Connector C306

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series (Black)

Connector Part Information

• | 12162000 (SWB)

• | 12186216 (LWB)

• | 2-Way M Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 882 | Right rear wheel speed signal-low | A | BRN | 882 | Right rear wheel speed signal-low
B | WHT | 883 | Right rear wheel speed signal-high | B | WHT | 883 | Right rear wheel speed signal-high

#### In-line Connector C308

Connector Part Information |

• | 12092249

• | 23-Way F ACT 280 Series (Black)

Connector Part Information

• | 12092248

• | 23-Way M ACT 280 Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 901 | Rear quarter window switch-close | A | BLK | 901 | Rear quarter window switch-close
B | LT GRN/BLK | 735 | Ambient air temperature sensor signal | B | LT GRN/BLK | 735 | Ambient air temperature sensor signal
C | DK GRN | 389 | Vehicle speed signal | C | DK GRN | 389 | Vehicle speed signal
D | -- | -- | Update | D | YEL | 136 | Fuel level input
E | BLK/WHT | 1896 | Power sliding door system switch signal | E | BLK/WHT | 1896 | Power sliding door system switch signal
F | TAN | 800 | UART serial data communication | F | TAN | 800 | UART serial data communication
G | GRY | 8 | Interior lamp dim signal | G | GRY | 8 | Interior lamp dim signal
H | YEL | 43 | Fused accessory feed | H | YEL | 43 | Fused accessory feed
J | BLK | 1550 | Ground | J | BLK | 1550 | Ground
K | BRN | 741 | Fused ignition 3 feed | K | BRN | 741 | Fused ignition 3 feed
L | -- | -- | Not Used | L | -- | -- | Not Used
M | GRY/BLK | 308 | Park lamp switch output-parklamps ON | M | GRY/BLK | 308 | Park lamp switch output-parklamps ON
N | ORN | 640 | Fused battery feed | N | ORN | 640 | Fused battery feed
P | -- | -- | Not Used | P | -- | -- | Not Used
R | LT GRN | 24 | Backup lamp feed | R | -- | -- | Update
S | GRY/BLK | 690 | Courtesy lamp control | S | GRY/BLK | 690 | Courtesy lamp control
T | -- | -- | Not Used | T | -- | -- | Not Used
U | LT BLU | 1894 | Power sliding door switch signal | U | LT BLU | 1894 | Power sliding door switch signal
V | -- | -- | Not Used | V | -- | -- | Not Used
W | DK BLU | 1393 | Courtesy lamps feed-protected battery | W | DK BLU | 1393 | Courtesy lamps feed-protected battery
X | PPL | 328 | Interior lamp override switch output | X | PPL | 328 | Interior lamp override switch output
Y | BRN | 541 | Fused ignition 3 feed | Y | BRN | 541 | Fused ignition 3 feed
Z | BRN | 902 | Rear quarter window switch-open | Z | BLK | 902 | Rear quarter window switch-open

#### In-line Connector C309

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series (Black)

Connector Part Information

• | 12162000 (SWB)

• | 12186216 (LWB)

• | 2-Way M Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 884 | Left rear wheel speed signal-high | A | BLK | 884 | Left rear wheel speed signal-high
B | WHT | 885 | Left rear wheel speed sensor-low | B | RED | 885 | Left rear wheel speed sensor-low

#### In-line Connector C313

Connector Part Information |

• | 12064749

• | 2-Way F Metri-Pack 150 Series (Black)

Connector Part Information

• | 12064750

• | 2-Way M Metri-Pack 480 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN/BLK | 340 | Fused battery feed | A | ORN | 340 | Fused battery feed
B | BLK | 550 | Ground | B | BLK | 550 | Ground

#### In-line Connector C314

Connector Part Information |

• | 12064749

• | 2-Way F Metri-Pack 150 Series (Black)

Connector Part Information

• | 12064750

• | 2-Way M Metri-Pack 480 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN/BLK | 340 | Fused battery feed | A | ORN | 340 | Fused battery feed
B | BLK | 550 | Ground | B | BLK | 550 | Ground

#### In-line Connector C326

Connector Part Information |

• | 12047785

• | 4-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047786

• | 4-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 8 | Interior Lights Dimming Feed | A | ORN | 8 | Interior Lights Dimming Feed
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | GRY | 150 | Interior Lights Dimming Ground | C | GRY | 150 | Interior Lights Dimming Ground
D | BLK/WHT | 906 | Rear Seat Audio (RSA) Enabled Signal | D | BLK/WHT | 906 | Rear Seat Audio (RSA) Enabled Signal

#### In-line Connector C328

Connector Part Information |

• | 12047886

• | 8-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12045688

• | 8-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT BLU | 115 | Video Audio Feed, Right (-) | A | LT BLU | 115 | Video Audio Feed, Right (-)
B | BLU | 46 | Radio Audio Feed, Right (+) | B | BLU | 46 | Radio Audio Feed, Right (+)
C | YEL | 116 | Radio Audio Feed, Left (+) | C | YEL | 116 | Radio Audio Feed, Left (+)
D | BRN | 199 | Radio Audio Feed, Left (-) | D | BRN | 199 | Radio Audio Feed, Left (-)
E | PPL | 115 | Video Audio Feed, Right (-) | E | PPL | 115 | Video Audio Feed, Right (-)
F | ORN | 46 | Radio Audio Feed, Right (+) | F | ORN | 46 | Radio Audio Feed, Right (+)
G | GRN | 116 | Radio Audio Feed, Left (+) | G | GRN | 116 | Radio Audio Feed, Left (+)
H | WHT | 199 | Radio Audio Feed, Left (-) | H | WHT | 199 | Radio Audio Feed, Left (-)

#### In-line Connector C397

Connector Part Information |

• | 12129489

• | 3-Way F Metri-Pack 280 Flexlock Series (Black)

Connector Part Information

• | 12129490

• | 3-Way M Metri-Pack 280 Flexlock Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 110 | Sunroof switch signal-close | A | ORN | 110 | Sunroof switch signal-close
B | BRN | 100 | Sunroof switch signal-open | B | BRN | 100 | Sunroof switch signal-open
C | WHT | 128 | Sunroof switch return | C | DK BLU | 128 | Sunroof switch return

#### In-line Connector C398

Connector Part Information |

• | 12020397

• | 3-Way F Metri-Pack 280 Series (Black)

Connector Part Information

• | 12020398

• | 3-Way M Metri-Pack 280 Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 541 | Fused ignition 3 feed | A | PNK | 541 | Fused ignition 3 feed
B | -- | -- | Not Used | B | -- | -- | Not Used
C | BLK | 650 | Ground | C | BLK | 650 | Ground

#### In-line Connector C400

Connector Part Information |

• | 12015199

• | 2-Way F Metri-Pack 280 Series (Natural)

Connector Part Information

• | 12015271

• | 2-Way M Metri-Pack 280 Series Sealed (Natural)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BLK | 450 | Ground | A | BLK | 450 | Ground
B | PPL | 293 | Rear defogger element feed | B | PPL | 293 | Rear defogger element feed

#### In-line Connector C401

Connector Part Information |

• | 12047785

• | 4-Way F Metri-Pack 150 Series (Black)

Connector Part Information

• | 12047786

• | 4-Way M Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RED/BLK | 780 | Door lock-key cylinder | A | RED/BLK | 780 | Door lock-key cylinder
B | ORN/BLK | 781 | Door unlock-key cylinder | B | ORN/BLK | 781 | Door unlock-key cylinder
C | GRY | 391 | Rear window wiper switch output | C | GRY | 391 | Rear window wiper switch output
D | DK GRN | 392 | Rear window washer pump motor feed | D | DK GRN | 392 | Rear window washer pump motor feed

#### In-line Connector C402

Connector Part Information |

• | 12047886

• | 8-Way F Metri-Pack 150 Flexlock Series Sealed (Black)

Connector Part Information

• | 12045688

• | 8-Way M Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 116 | Speaker return-left rear | A | YEL | 116 | Speaker return-left rear
B | BRN | 199 | Speaker feed-left rear | B | BRN | 199 | Speaker feed-left rear
C | BRN | 9 | Park lamp feed | C | BRN | 9 | Park lamp feed
D | WHT | 17 | Stop lamp switch output | D | WHT | 17 | Stop lamp switch output
E | YEL | 804 | Door ajar indicator lamp output | E | YEL | 804 | Door ajar indicator lamp output
F | DK BLU | 49 | Passenger door ajar switch signal | F | DK BLU | 49 | Passenger door ajar switch signal
G | DK BLU | 46 | Speaker feed-right rear | G | DK BLU | 46 | Speaker feed-right rear
H | LT BLU | 115 | Speaker return-right rear | H | LT BLU | 115 | Speaker return-right rear

#### In-line Connector C403

Connector Part Information |

• | 12020397

• | 3-Way F Metri-Pack 280 Series (Black)

Connector Part Information

• | 12020398

• | 3-Way M Metri-Pack 280 Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TAN | 294 | Passenger door lock motor feed-unlock | A | TAN | 294 | Passenger door lock motor feed-unlock
B | GRY | 295 | Passenger door lock motor feed-lock | B | GRY | 295 | Passenger door lock motor feed-lock
C | WHT | 393 | Rear window wiper motor feed | C | WHT | 393 | Rear window wiper motor feed

#### In-line Connector C405

Connector Part Information |

• | 12064769

• | 10-Way F Metri-Pack 150 Series (Natural)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (Natural)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1240 | Fused battery feed | A | ORN | 1240 | Fused battery feed
B | -- | -- | Not Used | B | -- | -- | Not Used
C | DK GRN | 19 | Tail/turn/stop lamp feed-right rear | C | DK GRN | 19 | Tail/turn/stop lamp feed-right rear
D | YEL | 18 | Tail/turn/stop lamp feed-left rear | D | YEL | 18 | Tail/turn/stop lamp feed-left rear
E | PNK | 39 | Fused ignition 1 feed | E | PNK | 39 | Fused ignition 1 feed
F | WHT | 17 | Stop lamp switch output | F | WHT | 17 | Stop lamp switch output
G | BRN | 9 | Park lamp feed | G | BRN | 9 | Park lamp feed
H | BLK | 1725 | Ground | H | BLK | 1725 | Ground
J-K | -- | -- | Not Used | J-K | -- | -- | Not Used

#### In-line Connector C407

Connector Part Information |

• | 12052848

• | 6-Way F Metri-Pack 150 Series (Black)

Connector Part Information

• | 12124107

• | 6-Way M Metri-Pack 150 Series (Black)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1240 | Fused battery feed | A | ORN | 1240 | Fused battery feed
B | BRN | 9 | Park lamp feed | B | BRN | 9 | Park lamp feed
C | YEL | 18 | Tail/turn/stop lamp feed-left rear | C | YEL | 18 | Tail/turn/stop lamp feed-left rear
D | DK GRN | 19 | Tail/turn/stop lamp feed-right rear | D | DK GRN | 19 | Tail/turn/stop lamp feed-right rear
E | WHT | 17 | Stop lamp switch output | E | WHT | 17 | Stop lamp switch output
F | BLK | 1725 | Ground | F | BLK | 1725 | Ground