For 1990-2009 cars

# CAMPAIGN: UPPER I/P GLOVE BOXOPENING EFFORT

#### Subject: PRODUCT SAFETY CAMPAIGN 91-C-09 UPPER INSTRUMENT PANEL GLOVE BOX OPENING EFFORT

#### MODELS AFFECTED: 1990-91 TRANS SPORT

#### TO: ALL PONTIAC DEALERS

The National Traffic and Motor Vehicle Safety Act, as amended, provides that each vehicle which is subject to a recall campaign of this type must be adequately repaired within a reasonable time after the owner has tendered it for repair. A failure to repair within sixty (60) days after tender of a vehicle is prima facie evidence of failure to repair within a reasonable time.

If the condition is not adequately repaired within a reasonable time, the owner may be entitled to an identical or reasonably equivalent vehicle at no charge or to a refund of the purchase price less a reasonable allowance for depreciation.

To avoid having to provide these burdensome solutions, every effort must be made to promptly schedule an appointment with each owner and to repair their vehicle as soon as possible. As you will see in reading the attached copy of the letter that is being sent to owners, the owners are being instructed to contact the Pontiac Customer Assistance Center if their dealer does not remedy the condition within five (5) days of the mutually agreed upon service date. If the condition is not remedied within a reasonable time, they are instructed on how to contact the National Highway Traffic Safety Administration.

#### DEFECT INVOLVED

General Motors has determined that certain 1990-91 Pontiac Trans Sport model vehicles fail to conform to Federal Motor Vehicle Safety Standard (FMVSS) 201, "Occupant Protection In Interior Impacts." Some of these vehicles were assembled with upper instrument panel (I/P) glove compartment doors which will not remain closed during certain load forces which can be experienced during a vehicle crash.

To correct this condition, dealers are to replace the current upper I/P glove compartment door with a redesigned upper I/P glove compartment door which incorporates a positive latch to keep the door closed should a vehicle crash occur.

#### VEHICLES INVOLVED

Involved are certain 1990-91 Pontiac Trans Sport model vehicles built within the following VIN breakpoints: Up To And Year Plant Beginning Including ---- ----- --------- --------- 1990 Tarrytown LT200001 LT500051 1991 Tarrytown MT200001 MT225752

Involved vehicles have been identified by Vehicle Identification Number Computer Listings. Computer listings contain the complete Vehicle Identification Number, owner name and address data, and are furnished to the involved dealers with the campaign bulletin. Owner name and address data furnished will enable dealers to follow-up with owners involved in this campaign.

These listings may contain owner names and addresses obtained from State Motor Vehicle Registration Records. The use of such motor vehicle registration data for any other purpose is a violation of law in several states. Accordingly, you are urged to limit the use of this listing to the follow-up necessary to complete this campaign. Any dealer not receiving a computer listing with the campaign bulletin has no involved vehicles currently assigned.

#### OWNER NOTIFICATION

Owners will be notified of this campaign on their vehicles by Pontiac Division (see copy of Owner Letter included with this bulletin).

#### DEALER CAMPAIGN RESPONSIBILITY

All unsold new vehicles in dealers' possession and subject to this campaign must be held and inspected/repaired per the Service Procedure of this campaign bulletin before owners take possession of these vehicles.

Dealers are to service all vehicles subject to this campaign at no charge to owners, regardless of mileage, age of vehicle, or ownership, from this time forward.

Owners of vehicles recently sold from your new vehicle inventory are to be contacted by the dealer, and arrangements made to make the required correction according to instructions contained in this bulletin.

In summary, whenever a vehicle subject to this campaign is taken into your new or used vehicle inventory, or it is in your dealership for service in the future, please take the steps necessary to be sure the campaign correction has been made before selling or releasing the vehicle.

This bulletin is notice to you that the new motor vehicles included in this campaign may not comply with the standard identified above. Under Section 108 of the National Traffic and Motor Vehicle Safety Act, it is illegal for a dealer to sell a new motor vehicle which the dealer knows does not comply with an applicable Federal Motor Vehicle Safety Standard. As a consequence, if you sell any of these motor vehicles without first performing the campaign correction, your dealership may be subject to a civil penalty up to $1,000 for each such sale.

#### PARTS INFORMATION

Parts required to complete this campaign are to be obtained from General Motors Service Parts Operation (GMSPO). To ensure that these parts are obtained as soon as possible, they should be ordered from GMSPO on a C.I.O. order with no special instruction code, but on advise code (2).

Part Quantity Description Number Per Vehicle ----------- ------ ----------- Upper Glove Compartment Door With Positive Latch: Medium Dark Grey 12518326 1 Medium Beachwood 12518325 1 Garnet Red 10217432 1

Retainer 10220565 1

#### SERVICE PROCEDURE

1. Open upper I/P glove compartment door, remove two (2) screws from hinge to door and remove door. Some doors may have shims at hinge. Remove shims and do not reinstall.

2. Install new door using screws removed in step 1.

3. Remove retainer from left side of glove box and install new retainer using same screw.

4. Install Campaign Identification Label.

#### CAMPAIGN IDENTIFICATION LABEL

Each vehicle modified in accordance with the instructions outlined in this Product Campaign Bulletin will require a "Campaign Identification Label." Each label provides a space to include the campaign number, the five digit dealer code of the dealer performing the campaign service, and the date the vehicle was campaigned. This information may be inserted with a typewriter or ballpoint pen. Install the label only on a clean, dry surface of the radiator baffle where it is readily visible. (Additional campaign labels are available on stationery order as Form 7201-709).

#### CLAIM INFORMATION

A separate repair order must be used for each vehicle. A completed warranty claim is to be kept as a permanent record of completion.

DEALERS SHOULD SUBMIT WARRANTY CLAIMS FOR CREDIT IN THEIR NORMAL MANNER WHEN THEY PERFORM THE SERVICE AS FOLLOWS: *Other Failure Labor Labor Labor Operation Code Operation Hours Hours --------- ------- --------- ----- ----- Install New Upper Glove Box Door 96 V7240 0.3 0.1

* In addition dealerships will receive 0.1 hours credit for dealer adminis- trative services associated with this campaign. The 0.1 hours allowance is to be entered in the "Other Labor Hours" field with each campaign repair listed for credit. This entry will not require authorization.

#### FAILURE CODE 96 MUST BE USED WITH THE LABOR OPERATION.

Parts required are to be listed in your warranty claim in the normal manner. Parts will be credited at dealer net plus 30% dealer handling allowance.

Dealers will be credited via Warranty Document or Terminal Transmission, whichever is their normal method of submission for payment. Claim must contain all information required and should list the labor operation as outlined.

#### RECORDING COMPLETION

Repairs submitted for vehicles not involved in the campaign will not be paid.

Campaign completion will be recorded from "PROPERLY COMPLETED AND PAID WARRANTY CLAIMS." Owners are being asked to present the owner reply card for identification to their dealer at the time they bring in their vehicle to have the campaign performed.

Dear Pontiac Owner:

This notice is sent to you in accordance with the requirements of the National Traffic and Motor Vehicle Safety Act.

REASON FOR THIS RECALL

General Motors has determined that certain 1990-91 Pontiac Trans Sport model vehicles fail to conform to Federal Motor Vehicle Safety Standard (FMVSS) 201, "Occupant Protection In Interior Impacts." Some of these vehicles were assembled with upper instrument panel (I/P) glove compartment doors which will not remain closed during certain load forces which can be experienced during a vehicle crash.

WHAT WE WILL DO

To correct this condition, your Pontiac dealer will replace the current upper glove compartment door with a redesigned upper glove compartment door which incorporates a latch to keep the door closed should a vehicle crash occur. This service will be performed for you at no charge.

WHAT YOU SHOULD DO

Please contact your Pontiac dealer as soon as possible to arrange a service date and so the dealer may order the necessary parts for the repair. Instructions for making this correction have been sent to your Pontiac Dealer and parts are available. The labor time necessary to perform this service correction is approximately fifteen (15) minutes. Please ask your dealer if you wish to know how much additional time will be needed to schedule and process your vehicle.

Your Pontiac dealer is best equipped to obtain parts and provide service to ensure your vehicle is corrected as promptly as possible. If, however, you take your vehicle to your dealer on the agreed service date, and he does not remedy this condition on that date, or within five (5) days, we recommend you contact the Pontiac Customer Assistance Center by calling: 1-800-762-2737.

After contacting your dealer and the Pontiac Customer Assistance Center, if you are still not satisfied that we have done our best to remedy this condition, without charge and within a reasonable time, you may wish to write the Administrator, National Highway Traffic Safety Administration, 400 Seventh Street, S. W., Washington, DC 20590 or call 1-800-424-9393 (Washington, DC residents use 366-0123).

The enclosed Campaign Owner Reply Card identifies your vehicle. Presentation of this card to your dealer will assist in making the correction in the shortest possible time. If you have sold or traded your vehicle, please let us know by completing the postage paid Owner Reply Card and returning it to us.

We are sorry to cause you this inconvenience; however, we have taken this action in the interest of your safety and continued satisfaction with our products.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.