For 1990-2009 cars

### Removal Procedure

1. Mark the location of the luggage carrier slats on the roof with masking tape.
2. Remove the luggage carrier slats. Refer to Exterior Trim Molding/Nameplate Replacement in Exterior Trim.
3. Remove the luggage carrier slats from the vehicle.

### Installation Procedure

1. Install the luggage carrier slats to the vehicle.
2. Align the luggage carrier slats with the masking tape applied to mark the slat locations.
3. Install the luggage carrier slats to the roof. Refer to Exterior Trim Molding/Nameplate Replacement in Exterior Trim.
4. Remove the masking tape.