For 1990-2009 cars

Rotate the tires and wheels at frequent intervals to equalize tire wear. Refer to Maintenance Schedule in Maintenance and Lubrication. Rotate the tires and wheels whenever uneven tire wear is noticed.

Radial tires tend to wear faster in the shoulder area, particularly the front tires. Radial tires in non-drive locations may develop an irregular wear pattern that may increase tire noise. This makes regular rotation especially necessary.

Refer to Wheel Removal and Wheel Installation .

After rotating the tires, adjust the tire pressures to specifications. Refer to Tire Inflation Pressure Specifications in Maintenance and Lubrication.