For 1990-2009 cars

### Removal Procedure

1. Use the following procedure in order to remove the switch mounting plate:

1.1. | Use a flat-bladed tool at the rear of the switch mounting plate in order to release the clip.

1.2. | Lift up in order to unsnap the mounting plate from the front door trim panel.

2. Disconnect the electrical connectors.
3. Unsnap the switch from the mounting plate.

### Installation Procedure

1. Install the switch to the mounting plate.
2. Connect the electrical connectors.
3. Install the switch mounting plate to the front door trim panel.

Insert the front edge into the trim panel and snap down the rear of the switch plate to the front door trim panel.