For 1990-2009 cars

### Removal Procedure

1. Remove the seat back cover. Refer to Front Seat Back Cushion Cover Replacement .
2. Remove the seat back pad from the frame (1).
3. Remove the lumbar mechanism. Refer to Front Seat Lumbar Support Replacement .
4. Remove the head restraint guides. Refer to Front Seat Head Restraint Replacement .
5. Remove the seat back frame (1).

### Installation Procedure

1. Install the seat back frame (1).
2. Install the head restraint guides. Refer to Front Seat Head Restraint Replacement .
3. Install the lumbar mechanism. Refer to Front Seat Lumbar Support Replacement .
4. Install the seat back pad to the frame (1).
5. Install the seat back cover. Refer to Front Seat Back Cushion Cover Replacement .