For 1990-2009 cars

#### Auxiliary Video Module (AVM) C1

Connector Part Information |

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 40 | Power Input | A | ORN | 40 | Power Input
B | DK GRN | 145 | Radio On Signal Input | B | DK GRN | 145 | Radio On Signal Input
C | WHT | 199 | Video Audio Input, Left (+) | C | WHT | 199 | Video Audio Input, Left (+)
D | YEL | 116 | Video Audio Input, Left (-) | D | YEL | 116 | Video Audio Input, Left (-)
E | -- | -- | Not Used | E | -- | -- | Not Used
F | LT BLU | 115 | Video Audio Input, Right (-) | F | LT BLU | 115 | Video Audio Input, Right (-)
G | BLU | 46 | Video Audio Input, Right (+) | G | BLU | 46 | Video Audio Input, Right (+)
H | BRN | -- | Video Signal Input (-) | H | BRN | -- | Video Signal Input (-)
J | GRY | -- | Video Signal Input (+) | J | GRY | -- | Video Signal Input (+)
K | BLK | 150 | Ground | K | BLK | 150 | Ground

#### Auxiliary Video Module (AVM) C2

Connector Part Information |

• | 12064762

• | 6-Way F Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12064763

• | 6-Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | -- | Video Signal Output (-) | A | WHT | -- | Video Signal Output (-)
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | ORN | 40 | Screen Position Input | C | ORN | 40 | Screen Position Input
D | RED | 40 | Ignition Power | D | RED | 40 | Ignition Power
E | PPL | 40 | Screen Power Feed (Output) | E | PPL | 40 | Screen Power Feed (Output)
F | YEL | -- | Video Signal Output (+) | F | YEL | 150 | Video Signal Output (+)

#### Auxiliary Video Module (AVM) C3

Connector Part Information |

• | 12064760

• | 4-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12064761

• | 4-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 40 | Power Output | A | ORN | 40 | Power Output
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | GRY | 8 | Interior Lights Dimming Input | C | GRY | 8 | Interior Lights Dimming Input
D | LT GRN | 145 | Radio On Signal Output | D | DK GRN | 145 | Radio On Signal Output

#### Auxiliary Video Module (AVM) C4

Connector Part Information |

• | 12064766

• | 8-Way F Metri-Pack 150 Series (BLU)

Connector Part Information

• | 12064767

• | 8-Way M Metri-Pack 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT BLU | 115 | Speaker Output (Video), Right (-) | A | LT BLU | 115 | Speaker Output (Video), Right (-)
B | DK BLU | 46 | Speaker Output (Video), Right (+) | B | DK BLU | 46 | Speaker Output (Video), Right (+)
C | YEL | 116 | Speaker Output (Video), Left (-) | C | YEL | 116 | Speaker Output (Video), Left (-)
D | BRN | 199 | Speaker Output (Video), Left (+) | D | BRN | 199 | Speaker Output (Video), Left (+)
E | PPL | 46 | Video Audio Channel Output, Left (+) | E | PPL | 46 | Video Audio Channel Output, Left (+)
F | GRN | 115/116 | Video Audio Channel Output (-) | F | GRN | 115/116 | Video Audio Channel Output (-)
G | WHT | 199 | Video Audio Channel Output, Right (+) | G | WHT | 199 | Video Audio Channel Output, Right (+)
H | BLK/WHT | 150 | Interior Lights Dimming Ground | H | WHT/BLK | 150 | Interior Lights Dimming Ground

#### Interface Module (IM)

Connector Part Information |

• | 12110259

• | 16-Way F Micro-Pack 100 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | LT BLU | 115 | Radio Audio Input (Right -)
A2 | DK BLU | 46 | Radio Audio Input (Right +)
A3 | YEL | 116 | Radio Audio Input (Left -)
A4 | BRN | 199 | Radio Audio Input (Left +)
A5 | LT GRN | 1011 | Rear Seat Audio System On Signal
A6 | GRY | 8 | Interior Lights Dimming Feed (Input)
A7 | -- | -- | Not Used
A8 | YEL | 43 | Ignition Power Input
B1 | LT BLU | 115 | Right Radio Rear Speaker Return (-)
B2 | DK BLU | 46 | Right Radio Rear Speaker Feed (+)
B3 | YEL | 116 | Left Radio Rear Speaker Return (-)
B4 | BRN | 199 | Left Radio Rear Speaker Feed (+)
B5 | BLK | 906 | Rear Seat Audio (RSA) Enabled Signal
B6 | BLK/WHT | 351 | Ground
B7 | -- | -- | Not Used
B8 | GRY/BLK | 308 | Pulsed Width Modulation (PWM) Input

#### Radio Rear Seat Audio Control

Connector Part Information |

• | 12110259

• | 16-Way F Micro-Pack 100 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | LT BLU | 115 | Speaker return-right rear
A2 | DK BLU | 46 | Speaker feed-right rear
A3 | YEL | 116 | Speaker return-left rear
A4 | BRN | 199 | Speaker feed-left rear
A5 | LT GRN | 1011 | RSA enable out
A6 | GRY | 8 | Interior lamp dim signal
A7 | -- | -- | Not Used
A8 | YEL | 43 | Fused accessory feed
B1 | LT BLU | 115 | Speaker return-right rear
B2 | DK BLU | 46 | Speaker feed-right rear
B3 | YEL | 116 | Speaker return-left rear
B4 | BRN | 199 | Speaker feed-left rear
B5 | BLK | 906 | RSA enable in
B6 | BLK/WHT | 351 | Ground-clean
B7 | -- | -- | Not Used
B8 | GRY/BLK | 308 | Park lamp switch output-park lamps ON

#### Second Seat Audio (SSA) Control

Connector Part Information |

• | 12064799

• | 12-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Interior Lights Dimming Feed (Input)
B | LT BLU | 115 | Radio Audio Input, Right (-)
C | DK BLU | 46 | Radio Audio Input, Right (+)
D | YEL | 116 | Radio Audio Input, Left (+)
E | BRN | 199 | Radio Audio Input, Left (-)
F | PPL | 115 | Video Audio Input, Right (-)
G | ORN | 46 | Video Audio Input, Right (+)
H | GRN | 116 | Video Audio Input, Left (-)
J | WHT | 199 | Video Audio Input, Left (+)
K | BLK | 150 | Ground
L | BLK/WHT | 906 | Rear Seat Audio (RSA) Enabled Input
M | GRY | 150 | Interior Lights Dimming Ground

#### Tape Retract Module (TRM)

Connector Part Information |

• | 12047785

• | 4-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 40 | B+ Feed
B | BLK | 150 | Ground
C | ORN | 40 | Ignition Feed
D | ORN | 40 | B+ Output (Switched)

#### Third Seat Audio (TSA) Control

Connector Part Information |

• | 12064799

• | 12-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 8 | Interior Lights Dimming Feed (Input)
B | LT BLU | 115 | Radio Audio Input, Right (-)
C | BLU | 46 | Radio Audio Input, Right (+)
D | YEL | 116 | Radio Audio Input, Left (+)
E | BRN | 199 | Radio Audio Input, Left (-)
F | PPL | 115 | Video Audio Input, Right (-)
G | ORN | 46 | Video Audio Input, Right (+)
H | GRN | 116 | Video Audio Input, Left (-)
J | WHT | 199 | Video Audio Input, Left (+)
K | BLK | 150 | Ground
L | BLK/WHT | 906 | Rear Seat Audio (RSA) Enabled Input
M | GRY | 150 | Interior Lights Dimming Ground

#### Video Entertainment System (VES) Relay

Connector Part Information |

• | 12129715

• | 6-Way F Metri-Pack 280 Series Flexlock (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | BLK | 150 | Ground
A2 | ORN | 40 | B+ Feed
B1-B2 | -- | -- | Not Used
C1 | ORN | 40 | B+ Feed (Relay Switched)
C2 | PNK/BLK | 39 | Ignition Feed

#### In-line Connector C326

Connector Part Information |

• | 12047785

• | 4-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047786

• | 4-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 8 | Interior Lights Dimming Feed | A | ORN | 8 | Interior Lights Dimming Feed
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | GRY | 150 | Interior Lights Dimming Ground | C | GRY | 150 | Interior Lights Dimming Ground
D | BLK/WHT | 906 | Rear Seat Audio (RSA) Enabled Signal | D | BLK/WHT | 906 | Rear Seat Audio (RSA) Enabled Signal

#### In-line Connector C328

Connector Part Information |

• | 12047886

• | 8-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12045688

• | 8-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT BLU | 115 | Video Audio Feed, Right (-) | A | LT BLU | 115 | Video Audio Feed, Right (-)
B | BLU | 46 | Radio Audio Feed, Right (+) | B | BLU | 46 | Radio Audio Feed, Right (+)
C | YEL | 116 | Radio Audio Feed, Left (+) | C | YEL | 116 | Radio Audio Feed, Left (+)
D | BRN | 199 | Radio Audio Feed, Left (-) | D | BRN | 199 | Radio Audio Feed, Left (-)
E | PPL | 115 | Video Audio Feed, Right (-) | E | PPL | 115 | Video Audio Feed, Right (-)
F | ORN | 46 | Radio Audio Feed, Right (+) | F | ORN | 46 | Radio Audio Feed, Right (+)
G | GRN | 116 | Radio Audio Feed, Left (+) | G | GRN | 116 | Radio Audio Feed, Left (+)
H | WHT | 199 | Radio Audio Feed, Left (-) | H | WHT | 199 | Radio Audio Feed, Left (-)

#### LH Radio Speaker

Connector Part Information |

• | 12052832

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 118 | Speaker feed-Left Front
B | TAN | 201 | Speaker return-Left Front

#### LH Radio Liftgate Speaker

Connector Part Information |

• | 12052832

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 116 |

• | Left Rear liftgate speaker feed

• | (UK6) Left Rear liftgate feed to radio rear speaker amplifier

B | BRN | 199 |

• | Left Rear liftgate speaker return

• | (UK6) Left Rear liftgate return to radio rear speaker amplifier

#### Remote CD Changer

Connector Part Information |

• | 12064980

• | 9-Way F Mircro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
7 | PNK | 314 | R14 In
8 | BRN/WHT | 230 | Interior lamp dim signal
9 | Bare | 2011 | Dim
10 | DK GRN/WHT | 368 | Right output
11 | BRN/WHT | 367 | Left output
12 | BLK/WHT | 372 | Audio signal return
13 | BLK/WHT | 351 | Power ground
14 | DK GRN | 835 | Entertainment and Comfort (E&C) serial data communication
15 | ORN | 640 | Fused battery feed

#### Radio C1

Connector Part Information |

• | 12047531

• | 10-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | 118 | Speaker return-Left Front
2 | TAN | 201 | Speaker feed-Left Front
3 | DK GRN | 117 | Speaker return-Right Front
4 | LT GRN | 200 | Speaker feed-Right F ront
5 | BLK/WHT | 351 | Ground
6 | GRY/BLK | 308 | Park lamp switch signal-park lamps ON
7 | BRN/WHT | 230 | Radio dimmer feed
8 | DK GRN | 145 | Radio ON Signal
9 | YEL | 43 | Fused power feed
10 | ORN | 640 | Fused battery feed

#### Radio C2

Connector Part Information |

• | 12065785

• | 10-Way F Micro-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
11 | -- | -- | Not Used
12 | BLK | 906 | RSA enable out
13 | LT GRN | 1011 | RSA In
14 | DK BLU | 1796 | Steering wheel controls input (Pontiac/Oldsmobile)
15 | DK GRN | 835 | Data link
16 | DK GRN | 389 | Vehicle speed sensor (VSS) (Chevrolet/Oldsmobile)
17 | LT BLU | 115 |

• | Right Rear liftgate speaker return

• | (UK6) Right Rear liftgate return to radio rear speaker amplifier

18 | DK BLU | 46 |

• | Right Rear liftgate speaker feed

• | (UK6) Right Rear liftgate feed to radio rear speaker amplifier

19 | YEL | 116 |

• | Left Rear liftgate speaker return

• | (UK6) Left Rear liftgate return to radio rear speaker amplifier

20 | BRN | 199 |

• | Left Rear liftgate speaker feed

• | (UK6) Left Rear liftgate feed to radio rear speaker amplifier

#### Radio C3

Connector Part Information |

• | 12064980

• | 9-Way F Mirco-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
7 | PNK | 314 | R14 out
8 | BRN/WHT | 230 | Interior lamp dim signal
9 | -- | -- | Not Used
10 | DK GRN/WHT | 368 | Right input
11 | BRN/WHT | 367 | Left input
12 | BLK/WHT | 372 | Audio signal return
13 | BLK/WHT | 351 | Power ground
14 | DK GRN | 835 | Entertainment and Comfort (E&C) serial data communication
15 | ORN | 640 | Fused battery feed out

#### RH Radio Liftgate Speaker

Connector Part Information |

• | 12052832

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 115 |

• | Right Rear liftgate speaker feed

• | (UK6) Right Rear liftgate feed to radio rear speaker amplifier

B | DK BLU | 46 |

• | Right Rear liftgate speaker return

• | (UK6) Right Rear liftgate return to radio rear speaker amplifier

#### RH Radio Speaker

Connector Part Information |

• | 12052832

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 117 | Speaker feed-Right Front
B | LT GRN | 200 | Speaker return-Right Front