For 1990-2009 cars

#### Tools Required

• | J 26958 Output Shaft Loading Tool

• | J 26958-10B Adaptor Plug

• | J 38385 Output Shaft Loading Tool Adaptor

Important: Install the bolts and tighten all bolts in order to prevent tool deflection during end play measurement.

Install the input clutch housing assembly end play tool as shown. You will use this tool in order to perform the selective washer check for the input clutch housing.