For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the front door window. Refer to Front Side Door Window Replacement .
4. Remove the weatherstrip from the door frame.

### Installation Procedure

1. Install the weatherstrip to the door frame.
2. Install the front door window. Refer to Front Side Door Window Replacement .
3. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .