For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Brake Transmission Shift Lock Control Actuator | Inside the steering column, near the ignition switch | -- | Tilt Wheel/Column Connector End Views
BTSI/TCC Brake Switch | Mounted to the brake pedal support, connector 2 of the stop lamp switch | -- | --
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | --
Stop Lamp Switch | Mounted to the brake pedal support | Antilock Brake System Component Views | Cruise Control Connector End Views
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Automatic Transmission Electronic Component Views | Powertrain Control Module Connector End Views
C101 (10 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, next to C103 and C181 | Antilock Brake System Component Views | Inline Harness Connector End Views
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Tilt Wheel/Column Component Views | Inline Harness Connector End Views
G113 | Engine compartment, left of the starter, along with the battery ground | Automatic Transmission Electronic Component Views | --
P100 | On the right side of the bulkhead, left of the right strut tower | HVAC Component Views | --
P101 | On the left side of the bulkhead, right of the left strut tower | Antilock Brake System Component Views | --
S106 | Engine harness, front left side of the engine compartment approximately 10 cm (4 in) from the PCM breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --