For 1990-2009 cars

Table 1: | 4T60-E, C/Hcar, trans. side
Table 2: | 4T60-E, Uvan, engine side

### Wiring Harness Assembly 7-way Connector, Transmission Side

#### 4T60-E, C/Hcar, trans. side

Connector Part Information |

• | 8683061

• | 7-way Metri-Pack 150 Series

• | Black

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | 0.8 BLK | 1222 | 1-2 Shift Solenoid (1-2 SS) Valve Control
B | 0.8 BLU | 1223 | 2-3 Shift Solenoid (2-3 SS) Valve Control
C | 0.8 BLK | 418 | Torque Converter Clutch Pulse Width Modulation Solenoid (TCC PWM Sol.) Valve Control
D | 0.8 TAN | 422 | Torque Converter Clutch Solenoid (TCC Sol.) Valve Control
E | 0.8 RED | 741 | Ignition Positive Voltage
F | 0.8 BRN | 1227 | Automatic Transmission Fluid Temperature (TFT) Sensor Input
G | 0.8 GRY | 452 | Sensor Ground

### Automatic Transmission Wiring Harness Assembly 7-way Connector, Engine Side

#### 4T60-E, Uvan, engine side

Connector Part Information | 12126467 7-way Metri-Pack 150 Series Black
--- | ---
Pin | Wire Color | Circuit No. | Function
A | 0.8 LT GRN | 1222 | 1-2 SS Valve Control
B | 0.8 YEL/BLK | 1223 | 2-3 SS Valve Control
C | 0.8 BRN | 418 | TCC PWM Sol. Valve Control
D | 0.5 TAN/BLK | 422 | TCC Sol. Valve Control
E | 0.5 PNK | 639 | Ignition Positive Voltage
F | 0.5 YEL/BLK | 1227 | TFT Sensor Signal
G | 0.8 BLK | 808 | Sensor Ground