For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Ashtray Lamp | Center of IP, mounted to the back of the ashtray | Power and Grounding Component Views in Wiring Systems | Lighting Systems Connector End Views
Auxiliary Heater-A/C Control (4 Door) | Part of the left rear armrest | HVAC Component Views in HVAC Systems with A/C-Manual | HVAC Connector End Views in HVAC Systems with A/C-Manual
Auxiliary Heater-A/C Control (5 Door) | Part of the rear roof console, behind the driver seat | HVAC Component Views in HVAC Systems with A/C-Manual | HVAC Connector End Views in HVAC Systems with A/C-Manual
Backup Lamps | Part of the taillamps | -- | --
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Cargo Lamp | Above the liftgate, on the roof headliner | Lighting Systems Component Views | Lighting Systems Connector End Views
Center High Mounted Stop Lamp (CHMSL) | Center, top of liftgate | Lighting Systems Component Views | Lighting Systems Connector End Views
Daytime Running Lamp (DRL) Ambient Light Sensor | Center of IP, secured to the upper trim pad, near the windshield defrost vent | -- | Lighting Systems Connector End Views
Daytime Running Lamps (DRL) Control Module | Right of the steering column, behind the IP | Lighting Systems Component Views | Lighting Systems Connector End Views
Dome Lamp | Center of the roof headliner | Lighting Systems Component Views | Lighting Systems Connector End Views
Driver Information Display | In the roof console | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Fog Lamp Relay | Engine compartment, in the underhood accessory wiring junction block | -- | --
Fog Lamps | On the front of the vehicle | -- | --
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | --
Hazard Lamp/Turn Signal Flasher | Below the IP, above the base of the steering column, left side of the steering column | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Headlamp Dimmer Switch | Part of the turn signal switch, mounted to the steering column | -- | --
Headlamp and IP Lamp Dimmer Switch | Left of the instrument cluster | Lighting Systems Component Views | Lighting Systems Connector End Views
Headlamps | Front of the vehicle | -- | --
Heater-A/C Control | Center of the IP, below the radio | HVAC Component Views in HVAC Systems with A/C-Manual | HVAC Connector End Views in HVAC Systems with A/C-Manual
Inflatable Restraint Steering Wheel Module Coil | Center of the steering wheel, behind the inflatable restraint steering wheel module | SIR Component Views in SIR | --
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Instrument Panel, Gages, and Console Connector End Views in HVAC Systems with A/C-Manual
Interior Lamp and Multi-function Switch | Center in front of the roof headliner | Lighting Systems Component Views | Lighting Systems Connector End Views
Interior Lamps Override Switch | Part of the interior lamp and multi-function switch, in front of the roof headliner | Lighting Systems Component Views | --
IP Compartment Lamp Switch | Inside of the IP compartment, part of the IP compartment lamp | -- | Lighting Systems Connector End Views
Left Fog Lamp | Front left side of the vehicle | Lighting Systems Component Views | Lighting Systems Connector End Views
Left Front Door Lock | Inside, rear end of the left front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Left Front Door Lock Switch | In the left front door armrest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Left Front Key Lock Switch | Inside the left front door, near the lock cylinder | -- | --
Left Front Park/Turn Lamp | In front of the vehicle, next to the headlamp | Lighting Systems Component Views | Lighting Systems Connector End Views
Left Front Roof Rail Reading Lamp | Left side of the headliner between the left B and left C-pillars | Lighting Systems Component Views | Lighting Systems Connector End Views
Left Front Side Marker Lamp | Front of the vehicle, left side | Lighting Systems Component Views | Lighting Systems Connector End Views
Left Front Window Switch | In the armrest of the left front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Left Headlamp | Front left side of the vehicle | Lighting Systems Component Views | Lighting Systems Connector End Views
Left Instrument Panel (IP) Courtesy Lamp | Below left side of the IP, near the park brake | -- | Lighting Systems Connector End Views
Left Rear Roof Rail Reading Lamp | Left side of the roof headliner, behind the left C-pillar and the left D-pillars | Lighting Systems Component Views | Lighting Systems Connector End Views
Left Sliding Door Jamb Switch | Mounted to the rear opening of the left rear side door | -- | --
Left Sunshade Lighted Vanity Mirror | Part of the left sunshade | -- | Lighting Systems Connector End Views
Left Taillamp | Rear of the vehicle, left side | Lighting Systems Component Views | Lighting Systems Connector End Views
Left Tail/Stop Lamp | Rear of the vehicle, inside the left taillamp | -- | --
License Lamps | Rear of the vehicle, above the license plate | Stationary Windows Component Views in Stationary Windows | Lighting Systems Connector End Views
Radio | Center of the IP console | Entertainment Component Views in Entertainment Systems | Entertainment Connector End Views in Entertainment Systems
Radio Control Switches | Left and right sides of the inflatable restraint steering wheel module | SIR Component Views in SIR | --
Radio Rear Seat Audio Control (4 Door) | Part of the left rear armrest | HVAC Component Views in HVAC Systems with A/C-Manual | Entertainment Connector End Views in Entertainment Systems
Radio Rear Seat Audio Control (5 Door) | Part of the rear roof console, above the driver seat | HVAC Component Views in HVAC Systems with A/C-Manual | Entertainment Connector End Views in Entertainment Systems
Radio Rear Seat Audio Control (WU3) | Part of the rear roof console, above the right passenger seat | -- | --
Rear Fog Lamps | On the rear of the vehicle | -- | --
Rear Window Wiper Motor | Center of the liftgate | Stationary Windows Component Views in Stationary Windows | Wiper/Washer Connector End Views in Wiper/Washer Systems
Rear Window Wiper/Washer and Multi-function Switch | Center of the IP, below the radio | Wiper/Washer Component Views in Wiper/Washer Systems | Wiper/Washer Connector End Views in Wiper/Washer Systems
Rear Window Wiper/Washer Switch | Part of the rear window wiper/washer and multi-function switch, center of the IP, below the radio | Wiper/Washer Component Views in WIper/Washer Systems | --
Relay Center | Right side of IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | Body Control System Component Views in Body Control System | Lighting Systems Connector End Views
Right Fog Lamp | Front right side of the vehicle | Lighting Systems Component Views | Lighting Systems Connector End Views
Right Front Door Lock | Inside, rear end of the right front door | Power Door Systems Component Views in Doors | --
Right Front Door Lock Switch | In the right front door armrest | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Right Front Park/Turn Lamp | Front of the vehicle, next to the headlamp | Lighting Systems Component Views | Lighting Systems Connector End Views
Right Front Side Marker Lamp | Front of the vehicle, right side | Lighting Systems Component Views | Lighting Systems Connector End Views
Right Front Window Switch | In the armrest of the right front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Right Headlamp | Front right side of the vehicle | Lighting Systems Component Views | Lighting Systems Connector End Views
Right IP Courtesy Lamp | Below the right side of the IP | -- | Lighting Systems Connector End Views
Right Rear Door Latch Release Actuator Switch | Middle of the right B-pillar | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Right Rear Roof Rail Reading Lamp | Right side of the roof headliner, between the right C-pillar and the right D-pillars | Lighting Systems Component Views | Lighting Systems Connector End Views
Right Sliding Door Jamb Switch | Mounted to the rear opening of the right rear side door | Power Door Systems Component Views in Doors | --
Right Sunshade Lighted Vanity Mirror | Part of the right sunshade | -- | Lighting Systems Connector End Views
Right Taillamp | Rear of the vehicle, right side | -- | Lighting Systems Connector End Views
Second Seat Audio (SSA) Control | Overhead console, right side of video screen | -- | --
Stop Lamp Switch | Mounted to the brake pedal support | Antilock Brake System Component Views in Antilock Brakes Systems | Cruise Control Connector End Views in Cruise Control
Theft Deterrent Relay | Part of the relay center, right side of the IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | Body Control System Component Views in Body Control System | --
Trailer Wiring Harness | Under the left right side of the vehicle, near the left rear wheelhouse | -- | --
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Automatic Transmission Electronic Component Views in Transmission | Engine Controls Connector End Views in Engine Controls
Turn Signal Lever (Cruise Control Switch) | Left side of the steering column, part of the turn signal switch | -- | --
Turn Signal Switch (& Headlamp Dimmer & Windshield Wiper & Windshield Washer) | Inside the steering column | -- | --
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Windshield Header Courtesy/Reading Lamp | Part of the roof console | Lighting Systems Component Views | Lighting Systems Connector End Views
C120 (3 cavities) | IP wiring harness to the forward lamp wiring harness, between the battery and the windshield fluid reservoir | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C205 (4 cavities) | IP wiring harness to the steering wheel radio control wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C302 (16 cavities) | Body wiring harness to the right front side door wiring harness, behind the right kick panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C303 (16 cavities) | Body wiring harness to the left front side door wiring harness, behind the left kick panel, left of the parking brake | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C308 (23 cavities) | Body wiring harness to the dome lamp wiring harness, inside the right B-pillar, behind the lower trim | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C400 (2 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C402 (8 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C405 (10 cavities) | Body wiring harness to the auto level control wiring harness, behind the left quarter panel, behind the left rear wheelhouse | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C407 (6 cavities) | Auto level control wiring harness to the trailer rear wiring harness, beneath the vehicle, near P403, near the left rear wheelhouse | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G101 | Front of the vehicle, right of the left headlamp, on the front upper crossmember | Harness Routing Views in Wiring Systems | --
G102 | Right side of the engine compartment, right inner fender, near the battery | Harness Routing Views in Wiring Systems | --
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views in Wiring Systems | --
G201 | Left side of the IP, secured on the underside of the cross car beam, above the park brake assembly | Harness Routing Views in Wiring Systems | --
G302 | Secured near the base of the right B-pillar | Harness Routing Views in Wiring Systems | --
G401 | Secured to the lower left D-pillar | Harness Routing Views in Wiring Systems | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views in Wiring Systems | --
P400 | Behind the right taillamp | Harness Routing Views in Wiring Systems | --
P401 | Behind the left taillamp | Harness Routing Views in Wiring Systems | --
P403 | Behind the left wheelhouse | Harness Routing Views in Wiring Systems | --
P406 | Between the right side of the liftgate and the roof | Harness Routing Views in Wiring Systems | --
P500 | Between the left A-pillar and the left front door | Harness Routing Views in Wiring Systems | --
P600 | Between the right A-pillar and the right front door | Harness Routing Views in Wiring Systems | --
S123 | Forward lamp harness, right front of the vehicle approximately 10 cm (4 in) from the right fog lamp breakout | -- | --
S124 | Forward lamp harness, left front of the vehicle approximately 7 cm (3 in) from the left fog lamp breakout | -- | --
S203 | IP harness, right side of the IP approximately 9 cm (4 in) from the radio breakout | -- | --
S204 | IP harness, right side of the IP approximately 10 cm (4 in) from the radio breakout | -- | --
S205 | IP harness, left side of the IP approximately 8 cm (3 in) from the hazard lamp/turn signal flasher breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --
S211 | IP harness, left side of the IP approximately 18 cm (7 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S213 | IP harness, center of IP approximately 68 cm (27 in) from the cigar lighter | -- | --
S215 | IP harness, left side of IP approximately 13 cm (5 in) from headlamp switch breakout | -- | --
S219 | IP harness, left side of the IP approximately 10 cm (4 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S221 | IP harness, left side of the IP approximately 4 cm (2 in) from the headlamp switch breakout | -- | --
S223 | IP harness, left side of the IP approximately 6 cm (2 in) from the radio and rear window wiper/washer and multi-function switch breakout | -- | --
S227 | IP harness, center of the IP approximately 4 cm (2 in) from the security indicator lamp breakout | -- | --
S230 | IP harness, right side of the IP approximately 4 cm (2 in) from the radio breakout | -- | --
S233 | IP harness, left side of the IP approximately 4 cm (2 in) from the radio breakout | -- | --
S242 | IP harness, left side of the IP approximately 14 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S247 | IP harness, center of the IP approximately 31 cm (12 in) from the radio | -- | --
S259 | IP harness, right side of the IP approximately 3 cm (1 in) from the cigar lighter breakout | -- | --
S264 | IP harness, right side of the IP approximately 16 cm (6 in) from the relay center breakout | -- | --
S272 | IP harness, right side of the IP approximately 2 cm (1 in) from the relay center breakout | -- | --
S284 | IP harness, right side of the IP approximately 6 cm (2 in) from P100 | -- | --
S303 | Body harness, front of the right B-pillar approximately 26 cm (10 in) from the inflatable restraint sensing and diagnostic module breakout | -- | --
S309 | Body harness, forward of the right front door approximately 7 cm (3 in) from the C302 breakout | -- | --
S320 | Body harness, near the base of the right B-pillar approximately 33 cm (13 in) forward of the right door lock switch plate (pillar mounted, plunger) breakout | -- | --
S325 | Body harness, front of the left B-pillar approximately 7 cm (3 in) from the left sliding door jamb switch breakout | -- | --
S331 | Body harness, front of the left B-pillar approximately 59 cm (23 in) from the G301 breakout | -- | --
S390 | Roof harness, overhead console approximately 10 cm (4 in) from the right sunshade lighted vanity mirror breakout | -- | --
S393 | Roof harness, right side of the overhead console approximately 20 cm (8 in) from the G302 breakout | -- | --
S395 | Roof harness, right side of the overhead console approximately 13 cm (5 in) from the G302 breakout | -- | --
S397 | Roof harness, right side of the overhead console approximately 7 cm (3 in) from the G302 breakout | -- | --
S403 | Body harness, left rear of the body on top of the wheel well approximately 13 cm (5 in) from the top and rear clips | -- | --
S405 | Body harness, left rear of the body approximately 4 cm (2 in) from the P401 breakout | -- | --
S406 | Body harness, left rear of the body approximately 17 cm (7 in) from the P401 breakout | -- | --
S407 | Body harness, left rear of the body approximately 13 cm (5 in) from the P401 breakout | -- | --
S411 | Body harness, left rear of the body approximately 7 cm (3 in) from the P401 breakout | -- | --
S415 | Body harness, left rear of the body approximately 11 cm (4 in) from the P401 breakout | -- | --
S419 | Body harness, left rear of the body approximately 21 cm (8 in) from the P401 breakout | -- | --
S431 | Body harness, left rear of the body approximately 4 cm (2 in) from the P401 breakout | -- | --
S435 | Body harness, left rear of the body approximately 26 cm (10 in) from the P401 breakout | -- | --
S441 | Auto level control harness, left rear of the body approximately 24 cm (9 in) from P403 | -- | --
S445 | Auto level control harness, left rear of the body approximately 16 cm (6 in) from P403 | -- | --
S457 | Liftgate harness, center of the liftgate approximately 7 cm (3 in) from the liftgate lock (door ajar switch) breakout | -- | --
S460 | Liftgate harness center of the liftgate approximately 7 cm (3 in) from the door lock cylinder switch breakout | -- | --
S504 | Left door harness, left door approximately 10 cm (4 in) from the left window switch breakout | -- | --
S506 | Left door harness, left door approximately 35 cm (3 in) from the left window switch | -- | --
S604 (w/AB5) | Right door harness, right door approximately 10 cm (4 in) from the right window switch breakout | -- | --
S604 (w/o AB5) | Right door harness, between P600 and the right front speaker breaker | -- | --
S606 | Right door harness, right door approximately 35 cm (13 in) from the right window switch | -- | --