For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel upper trim. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel and Console.
2. Remove the security system lamp. Refer to Lamp Replacement - Security Indicator in Theft Deterrent System.
3. Twist the daytime running lamp sensor counterclockwise in order to remove the sensor from the instrument panel upper trim.
4. Remove the daytime running lamp sensor from the wiring harness.

### Installation Procedure

1. Install the daytime running lamp sensor to the wiring harness.
2. Position the daytime running lamp sensor in the instrument panel upper trim and twist in order to secure.
3. Install the security system lamp. Refer to Lamp Replacement - Security Indicator in Theft Deterrent System.
4. Install the instrument panel upper trim. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel and Console.