For 1990-2009 cars

# PAINT INFORMATION

#### SUBJECT: PAINT INFORMATION

#### MODELS: 1994 PONTIAC PRODUCTS

THE FOLLOWING CHART PROVIDES PAINT INFORMATION ON 1994 PONTIAC PRODUCTS. THE PAINT TYPES LISTED BELOW THE MODELS INDICATE THE MATERIAL THE VEHICLE WAS MANUFACTURED WITH.

#### MODELS PAINT TYPE CODE# NAME WA# F H J N U W BASF PPG PPG DUP BASF DUP

08 MARY KAY PINK 9601 10 ARCTIC WHITE 9567 X 14 LT. GRAY MET. 9789 X X X X 16 BRIGHT WHITE 9753 X X X X X 18 DK. GREEN GRAY MET. 9795 X 26 MED. CLOISONNE MET. 127A X X X 30 MED. ADRIATIC MET. 9907 X X X X 31 MED. TEAL MET. 130A X 33 LT. DRIFTWOOD MET. 5322 X 34 LT. TEAL MET. 5323 X 35 DK. TEAL MET. 132A X 36 LT. ADRIATIC MET. 121A X 37 MED. TEAL BLUE MET. 146A X 41 BLACK 8555 X X X X X 43 BRIGHT AQUA MET. 9796 X X X 43 BRIGHT AQUA MET. 243A X 44 MED. MALACHITE MET. 9084 X 45 MED. GREEN PEARL 9539 X 48 DK. YELLOW GRN. MET. 9806 X 54 SUNFIRE YELLOW 9929 X 57 LT. BEIGE MET. 9805 X 71 MED. PATRIOT RED MET 9913 X 72 MED. GARNET RED MET. 8979 X X X X 80 MED. QUASAR MET. 5378 X 81 BRIGHT RED 8774 X X X X X X 84 HAWAIIAN ORCHID MET. 9802 X 91 PURPLE PEARL 9926 X X X

PAINT TYPES: DUP= DUPONT, PPG= PPG, BASF= BASF

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.