For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
7X Crankshaft Position (CKP) Sensor retaining bolt | 8 | -- | 70
24X Crankshaft Position (CKP) Sensor Bolts | 10 | 8 | --
A/C Refrigerant Pressure Sensor | 5 | -- | 44
Camshaft Position (CMP) Sensor Retaining Bolt | 10 | -- | 90
Crankshaft Balancer Bolt | 107 | 79 | --
Engine Coolant Temperature (ECT) Sensor | 30 | 22 | --
Engine Fuel Pipe Fittings | 17 | 13 | --
Engine Fuel Pipe Retaining Clip | 7.5 | -- | 67
Exhaust Gas Recirculation Valve | 30 | 22 | --
Engine Oil Level Sensor | 17-27 | 13-20 | --
Evaporative Emission Canister Retaining Bolts | 30 | 22 | --
EVAP Pipe Clip Screw | 5.8 | -- | 51
Front Fuel Tank Retaining Strap Nuts | 25 | 18 | --
Fuel Filler Pipe Hose Clamp | 2.5 | -- | 22
Fuel Filler Vent Hose Clamp | 2.5 | -- | 22
Fuel Pressure Regulator Screw | 8.5 | -- | 76
Fuel Rail Attaching Nuts or Bolts | 10 | -- | 89
Heated Oxygen Sensor(s) | 41 | 30 | --
IAC Valve Attaching Screws | 3 | -- | 27
Ignition Coil to Ignition Control Module screws | 4-5 | -- | 40
Ignition Control Module to Bracket Bolts | 8 | -- | 70
In-Pipe Fuel Filter Bracket Attaching Bolts | 27 | 20 | --
Knock Sensor(s) | 19 | -- | 14
Manifold Absolute Pressure (MAP) Sensor Retaining Bolt | 4-5 | -- | 40
Rear Fuel Tank Retaining Strap Bolts | 34 | 25 | --
Spark Plug(s) | 15 | 12 | --
Throttle Body Retaining Nuts or Bolts | 28 | 21 | --
TP Sensor Attaching Screws | 2 | -- | 18
Transaxle Range Switch Bolts | 28 | 20 | --
Upper Intake Manifold Studs or Bolts | 25 | 18 | --
Wheel Lug Nuts | 140 | 104 | --