For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | --
Rear Window Washer Pump | Engine compartment, mounted to the rear washer solvent container | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Rear Window Wiper Motor | Center of the liftgate | Stationary Windows Component Views in Stationary Windows | Wiper/Washer Connector End Views
Rear Window Wiper/Washer and Multi-function Switch | Center of the IP, below the radio | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Rear Window Wiper/Washer Switch | Part of the rear window wiper/washer and multi-function switch, center of the IP, below the radio | Wiper/Washer Component Views | --
Windshield Washer Pump | Engine compartment, mounted to the front washer solvent container | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Windshield Wiper Motor | Top right rear of the engine compartment | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Windshield Wiper/Washer Switch | Part of the turn signal switch, on the steering column | -- | Wiper/Washer Connector End Views
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C400 (2 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C401 (4 cavities) | Body wiring harness to the liftgate wiring harness, above the left rear side of the roof headliner, near P405 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C403 (3 cavities) | Body wiring harness to the liftgate wiring harness, above the left rear side of the roof headliner, near P405 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views in Wiring Systems | --
G401 | Secured to the lower left D-pillar | Harness Routing Views in Wiring Systems | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
P405 | Between the left side of the liftgate and the roof | Harness Routing Views in Wiring Systems | --
P406 | Between the right side of the liftgate and the roof | Harness Routing Views in Wiring Systems | --
S230 | IP harness, right side of the IP approximately 4 cm (2 in) from the radio breakout | -- | --
S245 | IP harness, right side of the IP approximately 5 cm (2 in) from the radio breakout, within the radio breakout | -- | --
S249 | IP harness, right side of the IP approximately 14 cm (6 in) from P100 | -- | --
S262 | IP harness, right side of the IP approximately 4 cm (2 in) from the blower motor resistor breakout | -- | --
S280 | IP harness, right side of the IP approximately 10 cm (4 in) from P100 | -- | --
S460 | Liftgate harness center of the liftgate approximately 7 cm (3 in) from the door lock cylinder switch breakout | -- | --